{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FVA71AMVEB / RZQSG71L3V1B","FVA100AMVEB / RZQSG100L9V1B","FVA125AMVEB / RZQSG125L9V1B","FVA140AMVEB / RZQSG140L9V1B"]
["Cooling capacity","Nom.","","كيلوواط","6.80","9.50","12.00","13.40"]
["تبريد المساحة","SEER","","","5.50","5.50","5.50","5.31"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","433","605","764","1,515"]
["","الاستطاعة","Pdesign","كيلوواط","6.80","9.50","12.00","13.40"]
["","فئة فعالية استهلاك الطاقة","","","A","A","A"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","كيلوواط","6.33","7.60","7.60","11.47"]
["","SCOP/A","","","3.86","4.01","3.85","3.69"]
["","فئة فعالية استهلاك الطاقة","","","A","A+","A"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","2,297","2,654","2,764","4,350"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","1,059","1,480","2,135"]
["","نسبة فعالية استهلاك الطاقة","","","3.21","3.21","2.81","2.51"]
["","عامل الأداء","","","3.61","3.61","3.41","3.41"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","C"]
["","","تدفئة","","A","A","B"]
["Heating capacity","Nom.","","كيلوواط","7.50","10.80","13.50","15.50"]
["Notes","","","","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - انظر الرسم المنفصل لنطاق التشغيل","(3) - انظر الرسم المنفصل لنطاق التشغيل","(3) - انظر الرسم المنفصل لنطاق التشغيل","(3) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]