{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A"]
[]
[]
[]
[]
["","","","","","FVA71AMVEB","FVA100AMVEB","FVA125AMVEB","FVA140AMVEB"]
["Cooling capacity","Total capacity","","Nom.","كيلوواط","","","12.10","13.40"]
["استطاعة التدفئة","الاستطاعة الإجمالية","","الإسمي","كيلوواط","","","13.5","15.5"]
["الغلاف","اللون","","","","أبيض صاف","أبيض صاف","أبيض صاف","أبيض صاف"]
["الأبعاد","الوحدة","","الارتفاع","مم","1850","1850","1850","1850"]
["","","","العرض","مم","600","600","600","600"]
["","","","العمق","مم","270","350","350","350"]
["الوزن","الوحدة","","","kg","42","50","50","50"]
["Fan","Air flow rate","التبريد","High","m³/min","18","28","28","30"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","16","25","26","28"]
["Fan","Air flow rate","التبريد","Low","m³/min","14","22","24","26"]
["","","التدفئة","High","m³/min","18","28","28","30"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","16","25","26","28"]
["Fan","Air flow rate","التدفئة","Low","m³/min","14","22","24","26"]
["مستوى طاقة الصوت","التبريد","","","ديسيبل أمبير","55","62","63","65"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","43","50","51","53"]
["مستوى ضغط الصوت","تبريد","","متوسط","ديسيبل أمبير","41","47","48","51"]
["Sound pressure level","Cooling","","Low","ديسيبل أمبير","38","44","46","48"]
["","Heating","","High","ديسيبل أمبير","43","50","51","53"]
["مستوى ضغط الصوت","تدفئة","","متوسط","ديسيبل أمبير","38","44","46","48"]
["Sound pressure level","Heating","","Nom.","ديسيبل أمبير","41","47","48","51"]
["وصلات الأنابيب","سائل","","القطر الخارجي","مم","9.52","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","مم","15.9","15.9","15.9","15.9"]
["","التصريف","","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["أنظمة التحكم","جهاز تحكم عن بُعد سلكي","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Hole protection rubber","","","","2","2","2","2"]
["","Cover","","","","1","1","1","1"]
["","Dew proof material","","","","1","1","1","1"]
["","Remote control wiring","","","","1","1","1","1"]
["","Bracket for installation","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Bush","","","","1","1","1","1"]
["","Installation pattern","","","","1","1","1","1"]
["","Insulation for fitting for gas pipe","","","","1","1","1","1"]
["","Insulation for fitting for liquid pipe","","","","1","1","1","1"]
["","Screws","","","","5","5","5","5"]
["","Tie-wraps","","","","5","5","5","5"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50/60","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","","","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]