{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FVQ100CVEB / RZQG71L9V1B","FVQ71CVEB / RZQG71L9V1B","FVQ140CVEB / RZQG100L9V1B","FVQ100CVEB / RZQG100L9V1B","FVQ125CVEB / RZQG125L9V1B","FVQ140CVEB / RZQG125L9V1B","FVQ140CVEB / RZQG140L9V1B"]
["Cooling capacity","Nom.","","كيلوواط","","6.8","","9.5","12.0","","13.4"]
["تبريد المساحة","SEER","","","6.31","6.23","5.61","5.61","5.61","5.61"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","378","383","593","593","749","749"]
["","الاستطاعة","Pdesign","كيلوواط","6.80","6.80","9.50","9.50","12.00","12.00"]
["","فئة فعالية استهلاك الطاقة","","","A++","A++","A+","A+","A+","A+"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","كيلوواط","6.33","6.33","11.30","11.30","11.30","11.30"]
["","SCOP/A","","","4.05","4.05","4.20","4.20","3.87","3.87"]
["","فئة فعالية استهلاك الطاقة","","","A+","A+","A+","A+","A","A"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","2,189","2,189","3,767","3,767","4,088","4,088"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","","1,010","","1,245","1,870","","2,085"]
["","نسبة فعالية استهلاك الطاقة","","","","3.37","","3.81","3.21","","3.21"]
["","عامل الأداء","","","","3.64","","4.14","3.70","","3.61"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","A","","A","A"]
["","","تدفئة","","","A","","A","A"]
["Heating capacity","Nom.","","كيلوواط","","7.5","","10.8","13.5","","15.5"]
["Notes","","","","","(1) - يتوافق الاستهلاك السنوي للطاقة مع توجيه الطاقة الملصق 2002/31/EC","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","","(2) - يتوافق SEER وSCOP مع EN 14825","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]