{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":7,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXG-L"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXG25L2V1B","FVXG35K2V1B / RXG35L2V1B","FVXG50K2V1B / RXG50L2V1B"]
["Cooling capacity","Min.","","كيلوواط","1.3","1.4","1.7"]
["","Max.","","كيلوواط","3.0","3.8","5.6"]
["","Nom.","","كيلوواط","2.5 (3)","3.5 (3)","5.0 (3)"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35","6.35"]
["","غاز","القطر الخارجي","mm","9.5","9.5","12.7"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","270","470","755"]
["","نسبة فعالية استهلاك الطاقة","","","4.63","3.72","3.31"]
["","عامل الأداء","","","4.42","3.75","3.69"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","A"]
["","","تدفئة","","A","A","A"]
["Heating capacity","Nom.","","كيلوواط","3.4 (4)","4.5 (4)","5.8 (4)"]
["","Min.","","كيلوواط","1.3","1.4","1.7"]
["","Max.","","كيلوواط","4.5","5.0","8.1"]
["Notes","","","","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)"]
["","","","","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)"]
["","","","","(3) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة‏، 19‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية للحوجلة الجافة‏، 24‏° مئوية للحوجلة الرطبة","(3) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة‏، 19‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية للحوجلة الجافة‏، 24‏° مئوية للحوجلة الرطبة","(3) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة‏، 19‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية للحوجلة الجافة‏، 24‏° مئوية للحوجلة الرطبة"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB"]
["","","","","(5) - 220 فولت","(5) - 220 فولت","(5) - 220 فولت"]
["","","","","(6) - 230 فولت","(6) - 230 فولت","(6) - 230 فولت"]
["","","","","(7) - 240 فولت","(7) - 240 فولت","(7) - 240 فولت"]
["","","","","(8) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(8) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(8) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected."]