{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":14,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RX-GV"]
[]
[]
[]
[]
["","","","","","RX20GV1B","RX25GV1B","RX35GV1B","RX50G2V1B","RX50G3V1B","RX60G2V1B","RX60G3V1B","RX71GV1B9","RX71GV1B"]
["Sound pressure level","Heating","","High","dBA","47","47","48","","","49","49","52","52"]
["","","","Low","dBA","","","","","","46","46","49","49"]
["","Cooling","","Low","dBA","","","","","","46","46","49","49"]
["","","","High","dBA","46","46","48","","","49","49","52","52"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1","1","1"]
["","سدادة المصرف","","","","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","1.5","1.5","2.1","","","3.1","3.1","4.8","4.8"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","0.74","0.74","1.0","","","1.5","1.5","2.3","2.3"]
["","النوع","","","","R-410A","R-410A","R-410A","","","R-410A","R-410A","R-410A","R-410A"]
["Piping connections","Level difference","IU - OU","Max.","م","12","12","12","","","20","20","20","20"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","","","0.020 (for piping length exceeding 10m)","0.020 (for piping length exceeding 10m)","0.020 (for piping length exceeding 10m)","0.020 (for piping length exceeding 10m)"]
["مستوى طاقة الصوت","التبريد","","","dBA","60","60","62","","","63","63","65","66"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","658","658","658","","","825","825","900","900"]
["","","","العمق","mm","275","275","275","","","300","300","320","320"]
["","","","الارتفاع","mm","550","550","550","","","735","735","770","770"]
["الوزن","الوحدة","","","kg","28","28","30","","","48","48","71","71"]
["Power supply","الطور","","","","1~","1~","1~","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","","","50","50","50","50"]
["","Voltage","","","فولت","220-240","220-240","220-240","","","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["الأبعاد","الوحدة","","الارتفاع","mm","","","","735","735"]
["","","","العرض","mm","","","","825","825"]
["","","","العمق","mm","","","","300","300"]
["الوزن","الوحدة","","","kg","","","","48","48"]
["ضاغط","نوع","","","","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","°مئوية مقياس الحوجلة الجافة","","","","-10","-10"]
["","","","Max.","°مئوية مقياس الحوجلة الجافة","","","","46","46"]
["","Heating","Ambient","Min.","°CWB","","","","-15","-15"]
["","","","Max.","°CWB","","","","18","18"]
["Sound pressure level","Cooling","","High","dBA","","","","47","47"]
["","","","Low","dBA","","","","44","44"]
["","Heating","","High","dBA","","","","48","48"]
["","","","Low","dBA","","","","45","45"]
["سائل تبريد","النوع","","","","","","","R-410A","R-410A"]
["","السعة","","","kg","","","","1.5","1.5"]
["","السعة","","","tCO2Eq","","","","3.1","3.1"]
["","GWP","","","","","","","2087.5","2087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","","","","30","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","","","","0.020 (for piping length exceeding 10m)","0.020 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","","","","20","20"]
["Standard Accessories","Drain socket","","","","","","","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","","","","1~","1~"]
["Power supply","Frequency","","","Hz","","","","50","50"]
["","Voltage","","","فولت","","","","220-240","220-240"]
["Notes","","","","","","","","(1) - 220 فولت","(1) - 220 فولت","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting"]
["","","","","","","","","(2) - 230 فولت","(2) - 230 فولت","(2) - 220 فولت","(2) - 220 فولت","(2) - 220 فولت","(2) - 220 فولت"]
["","","","","","","","","(3) - 240 فولت","(3) - 240 فولت","(3) - 230 فولت","(3) - 230 فولت","(3) - 230 فولت","(3) - 230 فولت"]
["Standard Accessories","تجويف المصرف","","","","","","","","","1","1","1","1"]
["Notes","","","","","","","","","","(4) - 240 فولت","(4) - 240 فولت","(4) - 240 فولت","(4) - 240 فولت"]
["","","","","","","","","","","(5) - يحتوي على غازات الاحتباس الحراري المفلورة","(5) - يحتوي على غازات الاحتباس الحراري المفلورة","(5) - يحتوي على غازات الاحتباس الحراري المفلورة","(5) - يحتوي على غازات الاحتباس الحراري المفلورة"]