{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":11,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXF-B"]
[]
[]
[]
[]
["","","","","","RXF20B5V1B","RXF25B5V1B","RXF50B2V1B","RXF50B5V1B","RXF60B2V1B","RXF60B5V1B"]
["الأبعاد","الوحدة","","الارتفاع","mm","550","550","734","734","734","734"]
["","","","العرض","mm","658","658","870","870","870","870"]
["","","","العمق","mm","275","275","373","373","373","373"]
["الوزن","الوحدة","","","kg","26","26","46.0","46.0","50.0","50.0"]
["Compressor","Type","","","","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["Sound pressure level","Cooling","","Nom.","ديسيبل أمبير","46","46","47","47","49","49"]
["","Heating","","Nom.","ديسيبل أمبير","47","47","49","49","49","49"]
["سائل تبريد","النوع","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","السعة","","","kg","0.55","0.55","0.90","0.90","1.15","1.15"]
["","السعة","","","tCO2Eq","0.37","0.37","0.61","0.61","0.78","0.78"]
["","GWP","","","","675.0","675.0","675","675","675","675"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","15","15","30","30","30","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","12","12","20","20","20","20"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1"]
["","Drain plug","","","","1","1","1","1","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","هرتز","50","50","50","50","50","50"]
["","Voltage","","","فولت","220-240","220-240","220-240","220-240","220-240","220-240"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Standard Accessories","Drain cap","","","","","","3","3","3","3"]