{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":16,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXJ-M"]
[]
[]
[]
[]
["","","","","","RXJ20M2V1B","RXJ20M3V1B","RXJ20M5V1B","RXJ25M2V1B","RXJ25M3V1B","RXJ25M5V1B","RXJ35M2V1B","RXJ35M3V1B","RXJ35M5V1B","RXJ50MV1B","RXJ50M2V1B"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","m³/min","29.3","","","29.3","","","29.3","","","38.5"]
["","","التدفئة","منخفض جداً","m³/min","25.6","","","25.6","","","25.6","","","34.3"]
["","","","منخفض جداً","cfm","1035","","","1035","","","1035","","","1359"]
["","","التدفئة","منخفض جداً","cfm","904","","","904","","","904","","","1211"]
["الأبعاد","الوحدة","","الارتفاع","مم","550","550","550","550","550","550","550","550","550","735","735"]
["","","","العرض","مم","765","765","765","765","765","765","765","765","765","825","825"]
["","","","العمق","مم","285","285","285","285","285","285","285","285","285","300","300"]
["الوزن","الوحدة","","","kg","34","32","32","34","32","32","34","32","32","44","44"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","دورة في الدقيقة","760","","","760","","","760","","","620"]
["","","التدفئة","منخفض جداً","دورة في الدقيقة","740","","","740","","","740","","","620"]
["Compressor","Type","","","","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","°مئوية مقياس الحوجلة الجافة","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Max.","°مئوية مقياس الحوجلة الجافة","46","46","46","46","46","46","46","46","46","46","46"]
["","Heating","Ambient","Min.","°CWB","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18","18","18","18","18","18","18","18","20"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","46","","","46","","","48","","","48","48"]
["","","","Nom.","ديسيبل أمبير","","46","46","","46","46","","49","49"]
["","","","Low","ديسيبل أمبير","","","","","","","","","","","45"]
["","Heating","","High","ديسيبل أمبير","47","","","47","","","48","","","48","48"]
["","","","Nom.","ديسيبل أمبير","","47","47","","47","47","","49","49"]
["","","","Low","ديسيبل أمبير","","","","","","","","","","","45"]
["سائل تبريد","النوع","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","السعة","","","kg","0.72","0.76","0.76","0.72","0.76","0.76","0.72","0.76","0.76","1.30","1.3"]
["","السعة","","","tCO2Eq","0.5","0.52","0.52","0.5","0.52","0.52","0.5","0.52","0.52","0.9","0.88"]
["","GWP","","","","675","675.0","675.0","675","675.0","675.0","675","675.0","675.0","675","675"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","20","20","20","20","20","20","20","20","20","30","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","15","15.0","15.0","15","15.0","15.0","15","15.0","15.0","20"]
["Standard Accessories","Installation manual","","","","1","1","","1","1","","1","1","","1"]
["","Drain plug","","","","1","1","","1","1","","1","1","","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220 فولت","","","(1) - 220 فولت","","","(1) - 220 فولت","","","(1) - 220 فولت"]
["","","","","","(2) - 230 فولت","","","(2) - 230 فولت","","","(2) - 230 فولت","","","(2) - 230 فولت"]
["","","","","","(3) - 240 فولت","","","(3) - 240 فولت","","","(3) - 240 فولت","","","(3) - 240 فولت"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Standard Accessories","Refrigerant charge label","","","","","1","","","1","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","1","","","1","","","1"]
["","General safety precautions","","","","","1","","","1","","","1"]