{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":11,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Sound pressure level","Heating","","High","ديسيبل أمبير","49","","","52"]
["","","","Low","ديسيبل أمبير","46","","","49"]
["","Cooling","","Low","ديسيبل أمبير","46","","","49"]
["","","","High","ديسيبل أمبير","49","","","52"]
["Standard Accessories","تجويف المصرف","","","","1","","","1"]
["","Installation manual","","","","1","Installation manual","1","1","Installation manual","1"]
["Refrigerant","Charge","","","TCO2Eq","3.1","","","4.8"]
["","GWP","","","","2,087.5","","","2,087.5"]
["","Charge","","","كغ","1.5","","","2.3"]
["","النوع","","","","R-410A","","","R-410A"]
["Piping connections","Level difference","IU - OU","Max.","م","20","","","20"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","","","0.02 (for piping length exceeding 10m)"]
["Sound power level","التبريد","","","ديسيبل أمبير","","","","65"]
["Compressor","Type","","","","Hermetically sealed swing compressor","","","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","825","","","900"]
["","","","العمق","mm","300","","","320"]
["","","","الارتفاع","mm","735","","","770"]
["الوزن","الوحدة","","","كغ","48","","","71"]
["Power supply","الطور","","","","1~","","","1~"]
["","Frequency","","","هرتز","50","","","50"]
["","Voltage","","","V","220-240","","","220-240"]
["Notes","","","","","(1) - SL: The silent fan level of the air flow rate setting","(1) - 220 فولت","","(1) - SL: The silent fan level of the air flow rate setting","(1) - 220 فولت"]
["","","","","","(2) - يحتوي على غازات الاحتباس الحراري المفلورة","(2) - 230 فولت","","(2) - يحتوي على غازات الاحتباس الحراري المفلورة","(2) - 230 فولت"]
["الأبعاد","الوحدة","","الارتفاع","mm","","735","735","","770","770"]
["","","","العرض","mm","","825","825","","900","900"]
["","","","العمق","mm","","300","300","","320","320"]
["الوزن","الوحدة","","","كغ","","48","48","","71","71"]
["Compressor","Type","","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","°CDB","","-10","-10","","-10","-10"]
["","","","Max.","°CDB","","46","46","","46","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","","-15","-15","","-15","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","","18","20","","18","20"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","","49","49","","52","52"]
["","","","Low","ديسيبل أمبير","","46","46","","49","49"]
["","Heating","","High","ديسيبل أمبير","","49","49","","52","52"]
["","","","Low","ديسيبل أمبير","","46","46","","49","49"]
["سائل تبريد","النوع","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","السعة","","","كغ","","1.5","1.5","","2.3","2.3"]
["","السعة","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","GWP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","","30","30","","30","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","","20","20","","20","20"]
["Standard Accessories","Drain plug","","","","","Drain plug","","","Drain plug"]
["وحدة التزويد بالطاقة","الطور","","","","","1~","1~","","1~","1~"]
["Power supply","Frequency","","","هرتز","","50","50","","50","50"]
["","Voltage","","","V","","220-240","220-240","","220-240","220-240"]
["Notes","","","","","","(3) - 240 فولت","","","(3) - 240 فولت"]
["Standard Accessories","Drain socket","","","","","","1","","","1"]