{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-K"]
[]
[]
[]
[]
["","","","","","RXS20K3V1B","RXS25K3V1B","RXS35K2V1B"]
["Sound pressure level","Heating","","High","dBA","47","47","48"]
["","Cooling","","High","dBA","46","46","48"]
["Standard Accessories","وصلة (تصريف)","","","","1","1"]
["","Installation manual","","","","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","2.1","2.1","2.5"]
["","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","1.0","1.0","1.2"]
["","النوع","","","","R-410A","R-410A","R-410A"]
["Fan motor","Speed","Cooling","منخفض جداً","rpm","780","780","780"]
["","","Heating","منخفض جداً","rpm","740","740","740"]
["Piping connections","Level difference","IU - OU","Max.","م","15","15","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","765","765","765"]
["","","","العمق","mm","285","285","285"]
["","","","الارتفاع","mm","550","550","550"]
["الوزن","الوحدة","","","kg","34","34","34"]
["Fan","Air flow rate","Heating","منخفض جداً","cfm","","","904"]
["","","Cooling","منخفض جداً","cfm","","","1,063"]
["Power supply","الطور","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت"]
["","","","","","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت"]
["","","","","","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت"]
["","","","","","(4) - SL: The silent fan level of the air flow rate setting","(4) - SL: The silent fan level of the air flow rate setting","(4) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["","","","","","(5) - يحتوي على غازات الاحتباس الحراري المفلورة","(5) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["Standard Accessories","سدادة المصرف","","","","","","1"]