{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":73,"n_cols":11,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Sound pressure level","Heating","","High","dBA","47","47","48","48"]
["","Cooling","","High","dBA","46","46","48","48"]
["Standard Accessories","غطاء المصرف","","","","1","1","","1"]
["","دليل التركيب","","","","1","1","1","1"]
["","ملصق الشحن بسائل التبريد","","","","1","1","1"]
["","ملصقات متعددة اللغات حول غازات الدفيئة المفلورة","","","","1","1","ملصقات متعددة اللغات حول غازات الدفيئة المفلورة"]
["Refrigerant","Charge","","","TCO2Eq","2.1","2.1","2.5","2.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","1.0","1.0","1.20","1.3"]
["","النوع","","","","R-410A","R-410A","R-410A","R-410A"]
["Fan motor","Speed","Cooling","منخفض جداً","rpm","780","780","780","790"]
["","","التدفئة","منخفض جداً","rpm","740","740","740","780"]
["Operation range","Cooling","Ambient","Max.","درجة بمقياس الحوجلة الجافة","46","46","46","46"]
["","","","Min.","درجة بمقياس الحوجلة الجافة","-10","-10","-10","-10"]
["","Heating","Ambient","Max.","°مئوية مقياس الحوجلة الرطبة","18","18","18","18"]
["","","","Min.","°مئوية مقياس الحوجلة الرطبة","-15","-15","-15","-15"]
["Piping connections","Level difference","IU - OU","Max.","م","","","15"]
["","Additional refrigerant charge","","","kg/m","","","0.020 (for piping length exceeding 10m)"]
["Dimensions","Unit","","العرض","mm","765","765","765","765"]
["","","","العمق","mm","285","285","285","285"]
["","","","الارتفاع","mm","550","550","550","550"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["الوزن","الوحدة","","","kg","34","34","34","39"]
["Fan","Air flow rate","التدفئة","منخفض جداً","cfm","904","904","904","960"]
["","","","منخفض جداً","m³/min","25.6","25.6","25.6","27.2"]
["","","التبريد","منخفض جداً","m³/min","30.1","30.1","30.1","30.6"]
["","","","منخفض جداً","cfm","1,063","1,063","1,063","1,080"]
["Power supply","الطور","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت"]
["","","","","","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت"]
["","","","","","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت"]
["","","","","","(4) - يحتوي على غازات الاحتباس الحراري المفلورة","(4) - يحتوي على غازات الاحتباس الحراري المفلورة","(4) - يحتوي على غازات الاحتباس الحراري المفلورة","(4) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["Standard Accessories","سدادة المصرف","","","","","","1"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","m³/min","","","","","48.9","45.0"]
["","","التدفئة","منخفض جداً","m³/min","","","","","43.1","46.3"]
["","","","منخفض جداً","cfm","","","","","1727","1589"]
["","","التدفئة","منخفض جداً","cfm","","","","","1522","1635"]
["الأبعاد","الوحدة","","الارتفاع","mm","","","","","735","735"]
["","","","العرض","mm","","","","","825","825"]
["","","","العمق","mm","","","","","300","300"]
["الوزن","الوحدة","","","kg","","","","","47","48"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","rpm","","","","","670"]
["","","التدفئة","منخفض جداً","rpm","","","","","670"]
["ضاغط","نوع","","","","","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","","","","","-10","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","","","","","46","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","","","","","-15","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","","","","","18","18"]
["Sound pressure level","Cooling","","High","dBA","","","","","48","49"]
["","","","Low","dBA","","","","","44","46"]
["","Heating","","High","dBA","","","","","48","49"]
["","","","Low","dBA","","","","","45","46"]
["سائل تبريد","النوع","","","","","","","","R-410A","R-410A"]
["","السعة","","","kg","","","","","1.7","1.5"]
["","السعة","","","tCO2Eq","","","","","3.5","3.1"]
["","GWP","","","","","","","","2087.5","2087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","","","","","30","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","","","","","0.020 (for piping length exceeding 10m)","0.020 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","","","","","20.0","20"]
["Standard Accessories","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","","","","","1~","1~"]
["Power supply","Frequency","","","Hz","","","","","50","50"]
["","Voltage","","","V","","","","","220-230-240","220-230-240"]
["Notes","","","","","","","","","","(1) - 230 فولت"]