{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Sound pressure level","Heating","","High","ديسيبل أمبير","","","48"]
["","Cooling","","High","ديسيبل أمبير","","","48"]
["Standard Accessories","دليل التركيب","","","","","","1"]
["","ملصق الشحن بسائل التبريد","","","","","","1"]
["","ملصقات متعددة اللغات حول غازات الدفيئة المفلورة","","","","","","1"]
["","سدادة تصريف (طرازات ذات مضخة الحرارة فقط)","","","","","","1"]
["Refrigerant","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Charge","","","kg","","","1.2"]
["","النوع","","","","","","R-410A"]
["Fan motor","Speed","Cooling","منخفض جداً","rpm","","","780"]
["","","Heating","منخفض جداً","rpm","","","740"]
["Operation range","Cooling","Ambient","Max.","°CDB","","","46"]
["","","","Min.","°CDB","","","-10"]
["","Heating","Ambient","Max.","°مئوية مقياس الحوجلة الرطبة","","","18"]
["","","","Min.","°مئوية مقياس الحوجلة الرطبة","","","-15"]
["Piping connections","Level difference","IU - OU","Max.","م","","","15"]
["","Additional refrigerant charge","","","kg/m","","","0.02 (for piping length exceeding 10m)"]
["Dimensions","Unit","","العرض","mm","","","765"]
["","","","العمق","mm","","","285"]
["","","","الارتفاع","mm","","","550"]
["Compressor","Type","","","","","","Hermetically sealed swing compressor"]
["الوزن","الوحدة","","","kg","","","34"]
["Fan","Air flow rate","Heating","منخفض جداً","cfm","","","904"]
["","","","منخفض جداً","m³/min","","","25.6"]
["","","Cooling","منخفض جداً","m³/min","","","30.1"]
["","","","منخفض جداً","cfm","","","1,063"]
["Power supply","الطور","","","","","","1~"]
["","Frequency","","","هرتز","","","50"]
["","Voltage","","","فولت","","","220-240"]
["Notes","","","","","","","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","m³/min","30.1","30.1"]
["","","التدفئة","منخفض جداً","m³/min","25.6","25.6"]
["","","","منخفض جداً","cfm","1063","1063"]
["","","التدفئة","منخفض جداً","cfm","904","904"]
["الأبعاد","الوحدة","","الارتفاع","mm","550","550"]
["","","","العرض","mm","765","765"]
["","","","العمق","mm","285","285"]
["الوزن","الوحدة","","","kg","34","34"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","rpm","780","780"]
["","","التدفئة","منخفض جداً","rpm","740","740"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-15","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18","18"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","46","46"]
["","Heating","","High","ديسيبل أمبير","47","47"]
["سائل تبريد","النوع","","","","R-410A","R-410A"]
["","السعة","","","kg","1.0","1.0"]
["","السعة","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","20","20"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","15","15"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~"]
["Power supply","Frequency","","","هرتز","50","50"]
["","Voltage","","","فولت","220-240","220-240"]
["Notes","","","","","(1) - 220 فولت"]
["","","","","","(2) - 230 فولت"]
["","","","","","(3) - 240 فولت"]
["Standard Accessories","Drain plug (only heat pump models)","","","","","1"]