{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B","RXZ35NV1B9","RXZ50NV1B","RXZ50NV1B9"]
["Sound pressure level","Heating","","High","ديسيبل أمبير","","","48","48","50","50"]
["","Cooling","","High","ديسيبل أمبير","","","48","48","49","49"]
["Standard Accessories","دليل التشغيل","","","","","","1","1","1","1"]
["","دليل التركيب","","","","","","1","1","1","1"]
["Refrigerant","GWP","","","","","","675","675","675","675"]
["","Charge","","","kg","","","1.34","1.34","1.34","1.34"]
["","النوع","","","","","","R-32","R-32","R-32","R-32"]
["Operation range","Cooling","Ambient","Max.","°CDB","","","43","43","43","43"]
["","","","Min.","°CDB","","","-10","-10","-10","-10"]
["","Heating","Ambient","Max.","°مئوية مقياس الحوجلة الرطبة","","","18","18","18","18"]
["","","","Min.","°مئوية مقياس الحوجلة الرطبة","","","-20","-20","-20","-20"]
["Piping connections","Level difference","IU - OU","Max.","م","","","8","8","8","8"]
["Dimensions","Unit","","العرض","mm","","","795","795","795","795"]
["","","","العمق","mm","","","300","300","300","300"]
["","","","الارتفاع","mm","","","693","693","693","693"]
["Compressor","Type","","","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["الوزن","الوحدة","","","kg","","","50","50","50","50"]
["Power supply","الطور","","","","","","1~","1~","1~","1~"]
["","Frequency","","","هرتز","","","50","50","50","50"]
["","Voltage","","","فولت","","","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت"]
["","","","","","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت"]
["","","","","","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت"]
["","","","","","","","(4) - يحتوي على غازات الاحتباس الحراري المفلورة","(4) - يحتوي على غازات الاحتباس الحراري المفلورة","(4) - يحتوي على غازات الاحتباس الحراري المفلورة","(4) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["الأبعاد","الوحدة","","الارتفاع","mm","693","693"]
["","","","العرض","mm","795","795"]
["","","","العمق","mm","300","300"]
["الوزن","الوحدة","","","kg","50","50"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","43","43"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-20","-20"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18","18"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","46","46"]
["","Heating","","High","ديسيبل أمبير","46","46"]
["سائل تبريد","النوع","","","","R-32","R-32"]
["","السعة","","","kg","1.34","1.34"]
["","السعة","","","tCO2Eq","0.9","0.9"]
["","GWP","","","","675","675"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","10","10"]
["Piping connections","Level difference","IU - OU","Max.","م","8","8"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~"]
["Power supply","Frequency","","","هرتز","50","50"]
["","Voltage","","","فولت","220-240","220-240"]