{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["الأبعاد","الوحدة","","الارتفاع","mm","734","734","734"]
["","","","العرض","mm","870","870","870"]
["","","","العمق","mm","373","373","373"]
["الوزن","الوحدة","","","kg","52","52","52"]
["Compressor","Type","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-20","-20","-20"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","52","52","52"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-21","-21","-21"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18","18","18"]
["مستوى طاقة الصوت","التبريد","","","dBA","62","63","64"]
["","التدفئة","","","dBA","62","63","64"]
["Sound pressure level","Cooling","","Nom.","dBA","48","49","50"]
["","Heating","","Nom.","dBA","48","49","50"]
["سائل تبريد","النوع","","","","R-32","R-32","R-32"]
["","السعة","","","kg","1.55","1.55","1.55"]
["","GWP","","","","675","675","675"]
["","السعة","","","tCO2Eq","1.05","1.05","1.05"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.52","12.7","12.7"]
["","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","50","50","50"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)","0.02 (for piping length exceeding 30m)","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","م","30","30","30"]
["Standard Accessories","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","(3) - يحتوي على غازات الاحتباس الحراري المفلورة","(3) - يحتوي على غازات الاحتباس الحراري المفلورة","(3) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["Standard Accessories","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]