{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":74,"n_cols":9,"rows_kept":74,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-MV1"]
[]
[]
[]
[]
["","","","","","RZAG71M7V1B","RZAG100M7V1B","RZAG125M7V1B","RZAG140M7V1B"]
["Sound pressure level","Heating","","Nom.","ديسيبل أمبير","","","","52"]
["","Cooling","","Nom.","ديسيبل أمبير","","","","51"]
["Standard Accessories","أغلفة برباط","","","","","","","2"]
["","دليل التركيب","","","","","","","1"]
["","ملصق سائل التبريد لقواعد غاز F","","","","","","","1"]
["","تدابير السلامة الوقائية العامة","","","","","","","1"]
["","ملصق الطاقة LOT10","","","","","","","1"]
["Refrigerant","Charge","","","TCO2Eq","","","","2.53"]
["","GWP","","","","","","","675"]
["","Charge","","","كغ","","","","3.75"]
["","النوع","","","","","","","R-32"]
["Piping connections","Liquid","","القطر الخارجي","مم","","","","9.52"]
["","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","","","","85"]
["","","نظام","بدون شحن","م","","","","40"]
["","","","مكافئ","م","","","","100"]
["","غاز","","القطر الخارجي","مم","","","","15.9"]
["","Level difference","IU - IU","Max.","م","","","","0.5"]
["","","IU - OU","Max.","م","","","","30.0"]
["","Additional refrigerant charge","","","kg/m","","","","See installation manual"]
["Sound power level","التبريد","","","ديسيبل أمبير","","","","70"]
["","التدفئة","","","ديسيبل أمبير","","","","70 (1)"]
["Compressor","Type","","","","","","","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","مم","","","","940"]
["","","","العمق","مم","","","","320"]
["","","","الارتفاع","مم","","","","1,430"]
["الوزن","الوحدة","","","كغ","","","","92"]
["Power supply","الطور","","","","","","","1~"]
["","Frequency","","","Hz","","","","50"]
["","Voltage","","","V","","","","220-240"]
["Notes","","","","","","","","(1) - حسب ENER Lot 21"]
["","","","","","","","","(2) - المعايير الفنية الأوروبية / الدولية التي تحدد حدود التيارات التوافقية التي تنتجها المعدات المتصلة بنظام الجهد المنخفض العام مع تيار دخل أكبر من 16 أمبير و أصغر أو يساوي 75 أمبير لكل طور."]
["","","","","","","","","(3) - Ssc: قوة الماس الكهربائى"]
["","","","","","","","","(4) - يقوم المقياس التقني الأوروبي/العالمي بتحديد قيود على التيارات التوافقية الناتجة عن الأجهزة الموصولة بنظاو الفولتية المنخفضة العامة بتيار دخل ≤ 16 آمبير  لكل طور."]
["الأبعاد","الوحدة","","الارتفاع","مم","990","1430","1430"]
["","","","العرض","مم","940","940","940"]
["","","","العمق","مم","320","320","320"]
["الوزن","الوحدة","","","كغ","70","92","92"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-20","-20","-20"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","52","52","52"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-20","-20","-20"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18.0","18.0","18.0"]
["مستوى طاقة الصوت","التبريد","","","ديسيبل أمبير","64","66","69"]
["Sound pressure level","Cooling","","Nom.","ديسيبل أمبير","46","47","50"]
["","Heating","","Nom.","ديسيبل أمبير","49","51","52"]
["سائل تبريد","النوع","","","","R-32","R-32","R-32"]
["","السعة","","","كغ","2.95","3.75","3.75"]
["","GWP","","","","675","675","675"]
["","السعة","","","tCO2Eq","1.99","2.53","2.53"]
["وصلات الأنابيب","سائل","","القطر الخارجي","مم","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","مم","15.9","15.9","15.9"]
["","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","55","85","85"]
["","","نظام","مكافئ","م","75","100","100"]
["","","","بدون شحن","م","40","40","40"]
["Piping connections","Additional refrigerant charge","","","kg/m","See installation manual","See installation manual","See installation manual"]
["","Level difference","IU - OU","Max.","م","30.0","30.0","30.0"]
["","","IU - IU","Max.","م","0.5","0.5","0.5"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["تيار - 50 هرتز","قيمة الأمبير القصوى للفاصمة (MFA)","","","آمبير","20","32","32"]
["مستوى طاقة الصوت","التدفئة","","","ديسيبل أمبير","","","69 (1)"]
["Notes","","","","","","","(1) - حسب ENER Lot 21"]