{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":8,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R / ARXM-A"]
[]
[]
[]
[]
["","","","","ATXM25R2V1B / ARXM25A5V1B","ATXM25R5V1B / ARXM25A5V1B","ATXM35R2V1B / ARXM35A5V1B","ATXM35R5V1B / ARXM35A5V1B"]
["Cooling capacity","Min.","","kW","0.9","0.9","0.9","0.9"]
["","Nom.","","kW","2.5","2.5","3.5","3.5"]
["","Max.","","kW","3.8","3.8","4.4","4.4"]
["Heating capacity","Min.","","kW","0.8","0.8","0.8","0.8"]
["","Nom.","","kW","2.8","2.8","4","4"]
["","Max.","","kW","5","5","5.5","5.5"]
["Nominal efficiency","EER","","","5.1","5.1","4.5","4.5"]
["","COP","","","5","5","4.45","4.45"]
["","Annual energy consumption","","kWh","245","245","389","389"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","A","A","A","A"]
["Space cooling","Energy efficiency class","","","A+++","A+++","A+++","A+++"]
["","Capacity","Pdesign","kW","2.5","2.5","3.5","3.5"]
["","SEER","","","9.3","9.3","9.1","9.1"]
["","Annual energy consumption","","kWh/a","94","94","135","135"]
["Space heating (Average climate)","Energy efficiency class","","","A+++","A+++","A+++","A+++"]
["","Capacity","Pdesign","kW","2.4","2.4","2.5","2.5"]
["","SCOP/A","","","5.15","5.15","5.15","5.15"]
["","Pdh Heating capacity at -10°","","kW","2.4","2.4","2.5","2.5"]
["","Annual energy consumption","","kWh/a","652","652","679","679"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notes","","","","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]