{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Maximum number of connectable indoor units","","","","","32"]
["Ambient temperature","Relative humidity <","","","%","85"]
["Power input","kW","","","","0.015 (1)"]
["Communication","DIII-NET","","Quantity","","1"]
["","","","Remark","","DIII-NET (F1F2)"]
["","Ethernet","","Quantity","","1"]
["","Input terminal","Digital","Quantity","","4"]
["Dimensions","Unit","","Width","mm","384"]
["","","","Depth","mm","92"]
["","","","Height","mm","136"]
["Maximum number of connectable outdoor units","","","","","7"]
["Power supply","Frequency","","","Hz","50/60"]
["","Voltage","","","V","110-240 AC"]
["Notes","","","","","(1) - Includes the power input of the WAGO power supply, the CPU module and the I/O module"]
["","","","","","(2) - The dimensions include the WAGO power supply, the CPU modulen, the I/O module and the necessary space in between the different parts"]
["","","","","","(3) - The dimension of the optional screen are: height: 209mm, width: 123mm, depth: 8.5mm"]