{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":15,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKEXV"]
[]
[]
[]
[]
["","","","","","EKEXV100","EKEXV125","EKEXV140","EKEXV200","EKEXV250","EKEXV400","EKEXV50","EKEXV500","EKEXV63","EKEXV80"]
["Dimensions","Unit","","Height","mm","401","401","401","401","401","401","401","401","401","401"]
["","","","Width","mm","215","215","215","215","215","215","215","215","215","215"]
["","","","Depth","mm","78","78","78","78","78","78","78","78","78","78"]
["Weight","Unit","","","kg","2.9","2.9","2.9","2.9","2.9","2.9","2.9","2.9","2.9","2.9"]
["Operation range","Cooling","","Min.","°CDB","-5","-5","-5","-5","-5","-5","-5","-5","-5","-5"]
["","","","Max.","°CDB","46","46","46","46","46","46","46","46","46","46"]
["Sound pressure level","Nom.","","","dBA","45","45","45","45","45","45","45","45","45","45"]
["Piping connections","Liquid","","Type","","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection"]
["","","","OD","mm","9.52","9.52","9.52","9.52","9.52","12.70","6.35","15.90","9.52","9.52"]
["","Gas","","Type","","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection"]
["","","","OD","mm","9.52","9.52","9.52","9.52","9.52","9.52","6.35","9.52","9.52","9.52"]
["","Piping length","System","Chargeless","m","0","0","0","0","0","0","0","0","0","0"]
["","Level difference","IU - IU","Max.","","See manual, depends on the outdoor unit","See manual, depends on the outdoor unit","See manual, depends on the outdoor unit","See manual, depends on the outdoor unit","See manual, depends on the outdoor unit","See manual, depends on the outdoor unit","See manual, depends on the outdoor unit","See manual, depends on the outdoor unit","See manual, depends on the outdoor unit","See manual, depends on the outdoor unit"]
["Notes","","","","","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit","(2) - Minimum and maximum piping length refer to the piping between the expansion valve kit (EKEXV) and the air handling unit"]