{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-DVM / RZQ-KVJ"]
[]
[]
[]
[]
["","","","FBQ20DVM / RZQ20KCVJK","FBQ24DVM / RZQ24KCVJK","FBQ36DVM / RZQ36KCVJK","FBQ45DVM / RZQ45KCVJK"]
["Cooling capacity","Min.","kW","3.3 (1)","3.3 (1)","5.0 (1)","6.0 (1)"]
["","Max.","kW","7.1 (1)","8.1 (1)","11.4 (1)","14.3 (1)"]
["","Nom.","kW","5.9 (1), 5.0 (2)","6.5 (1), 5.3 (2)","9.4 (1), 8.0 (2)","11.4 (1), 9.1 (2)"]
["Nominal efficiency","EER","","3.28 (3), 11.18 (4)","2.95 (3), 10.08 (4)","3.11 (3), 10.62 (4)","2.79 (3), 9.53 (4)"]
["","COP","","3.68 (5), 12.57 (6)","3.48 (5), 11.87 (6)","3.67 (5), 12.51 (6)","3.68 (5), 12.57 (6)"]
["Heating capacity","Nom.","kW","7.0","8.0","11.0","14.0"]
["","Min.","kW","3.5","3.5","5.6","6.0"]
["","Max.","kW","8.0","9.0","12.8","16.2"]
["Notes","","","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1"]
["","","","(2) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3","(2) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3","(2) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3","(2) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3"]
["","","","(3) - EER: W/W","(3) - EER: W/W","(3) - EER: W/W","(3) - EER: W/W"]
["","","","(4) - EER: Btu/h/W","(4) - EER: Btu/h/W","(4) - EER: Btu/h/W","(4) - EER: Btu/h/W"]
["","","","(5) - COP: W/W","(5) - COP: W/W","(5) - COP: W/W","(5) - COP: W/W"]
["","","","(6) - COP: Btu/h/W","(6) - COP: Btu/h/W","(6) - COP: Btu/h/W","(6) - COP: Btu/h/W"]
["","","","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]