{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-DVM / RZQ-LYA"]
[]
[]
[]
[]
["","","","FBQ45DVM / RZQ45LUYAK","FBQ48DVM / RZQ48LUYAK"]
["Cooling capacity","Min.","kW","6.0 (1)","6.2 (1)"]
["","Max.","kW","14.3 (1)","15.8 (1)"]
["","Nom.","kW","11.4 (1), 9.1 (2)","11.7 (1), 9.4 (2)"]
["Nominal efficiency","EER","","2.79 (3), 9.53 (4)","2.73 (3), 9.31 (4)"]
["","COP","","3.68 (5), 12.57 (6)","3.30 (5), 11.27 (6)"]
["Heating capacity","Nom.","kW","14.0","15.2"]
["","Min.","kW","6.0","6.2"]
["","Max.","kW","16.2","18.1"]
["Notes","","","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1"]
["","","","(2) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3","(2) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3"]
["","","","(3) - EER: W/W","(3) - EER: W/W"]
["","","","(4) - EER: Btu/h/W","(4) - EER: Btu/h/W"]
["","","","(5) - COP: W/W","(5) - COP: W/W"]
["","","","(6) - COP: Btu/h/W","(6) - COP: Btu/h/W"]
["","","","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]