{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":9,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-DVM"]
[]
[]
[]
[]
["","","","","FBQ20DAVMK","FBQ24DAVMK","FBQ36DAVMK","FBQ45DAVMK","FBQ48DAVMK"]
["Standard Accessories","Operation manual","","","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual"]
["","Installation manual","","","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual"]
["","Drain hose","","","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose"]
["","Hose band","","","Hose band","Hose band","Hose band","Hose band","Hose band"]
["","Sealing pads","","","Sealing pads","Sealing pads","Sealing pads","Sealing pads","Sealing pads"]
["","Clamps","","","Clamps","Clamps","Clamps","Clamps","Clamps"]
["","Washer","","","Washer","Washer","Washer","Washer","Washer"]
["","Screws","","","Screws","Screws","Screws","Screws","Screws"]
["","Insulation for fitting","","","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting"]
["","Clamp metal","","","Clamp metal","Clamp metal","Clamp metal","Clamp metal","Clamp metal"]
["","Air discharge flange","","","Air discharge flange","Air discharge flange","Air discharge flange","Air discharge flange","Air discharge flange"]
["","Air suction flange","","","Air suction flange","Air suction flange","Air suction flange","Air suction flange","Air suction flange"]
["Piping connections","Liquid","OD","mm","9.52","9.52","9.52","9.52","9.52"]
["","Gas","OD","mm","15.9","15.9","15.9","15.9","15.9"]
["","Drain","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Dimensions","Unit","Width","mm","1,000","1,000","1,400","1,400","1,400"]
["","","Depth","mm","700","700","700","700","700"]
["","","Height","mm","300","300","300","300","300"]
["Weight","Unit","","kg","36","36","46","46","46"]
["Fan","External static pressure","High","Pa","200","200","200","200","200"]
["","","Nom.","Pa","50","50","50","50","50"]
["Power supply","Phase","","","1~","1~","1~","1~","1~"]
["","Frequency","","Hz","60","60","60","60","60"]
["","Voltage","","V","230","230","230","230","230"]
["Notes","","","","(1) - The air filter is not a standard accessory, but please mount it in the duct system of the suction side. Select its colorimetric method (gravity method) 50% or more.","(1) - The air filter is not a standard accessory, but please mount it in the duct system of the suction side. Select its colorimetric method (gravity method) 50% or more.","(1) - The air filter is not a standard accessory, but please mount it in the duct system of the suction side. Select its colorimetric method (gravity method) 50% or more.","(1) - The air filter is not a standard accessory, but please mount it in the duct system of the suction side. Select its colorimetric method (gravity method) 50% or more.","(1) - The air filter is not a standard accessory, but please mount it in the duct system of the suction side. Select its colorimetric method (gravity method) 50% or more."]
["","","","","(2) - External static pressure: initial setting is nominal","(2) - External static pressure: initial setting is nominal","(2) - External static pressure: initial setting is nominal","(2) - External static pressure: initial setting is nominal","(2) - External static pressure: initial setting is nominal"]