{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / AZQS-BY1 UK"]
[]
[]
[]
[]
["","","","","FCQG100FVEB / AZQS100B7Y1B UK","FCQG125FVEB / AZQS125B7Y1B UK","FCQG140FVEB / AZQS140B7Y1B UK"]
["Cooling capacity","Nom.","","kW","9.5","12.1","13.0"]
["Space cooling","SEER","","","5.50"]
["","Annual energy consumption","","kWh/a","605"]
["","Capacity","Pdesign","kW","9.50"]
["","Energy efficiency class","","","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","7.60"]
["","SCOP/A","","","3.85"]
["","Energy efficiency class","","","A"]
["","Annual energy consumption","","kWh/a","2,764"]
["Nominal efficiency","EER","","","3.21","3.10","2.81"]
["","Annual energy consumption","","kWh","1,480","1,952","2,313"]
["","COP","","","3.50","3.41","3.30"]
["","Energy labeling Directive","Cooling","","A","B"]
["","","Heating","","B","B"]
["Heating capacity","Nom.","","kW","10.8","13.5","15.5"]
["Notes","","","","(1) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","(1) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","(1) - Annual energy consumption is according to Energy labeling directive 2002/31/EC"]
["","","","","(2) - SEER and SCOP are according to EN 14825","(2) - SEER and SCOP are according to EN 14825","(2) - SEER and SCOP are according to EN 14825"]
["","","","","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]