{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RXL-K"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / RXL35K2V1B","FCQG50FVEB / RXL50K2V1B"]
["Cooling capacity","Min.","","kW","1.3","1.6"]
["","Max.","","kW","4.0","5.7"]
["","Nom.","","kW","3.40","5.00"]
["Space cooling","SEER","","","5.65","6.11"]
["","Annual energy consumption","","kWh/a","217","286"]
["","Capacity","Pdesign","kW","3.50","5.00"]
["","Energy efficiency class","","","A+","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","3.32","4.36"]
["","SCOP/A","","","4.65","4.18"]
["","Energy efficiency class","","","A++","A+"]
["","Annual energy consumption","","kWh/a","1,001","1,463"]
["Nominal efficiency","EER","","","3.70","3.57"]
["","Annual energy consumption","","kWh","460","700"]
["","COP","","","3.56","3.87"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","B","A"]
["Heating capacity","Nom.","","kW","4.20","6.00"]
["","Min.","","kW","1.3","1.6"]
["","Max.","","kW","5.2","6.5"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]