{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RXS-K"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / RXS35K2V1B","FCQG50FVEB / RXS50K2V1B"]
["Cooling capacity","Nom.","","kW","3.40","5.00"]
["Space cooling","SEER","","","5.34","5.89"]
["","Annual energy consumption","","kWh/a","230","297"]
["","Capacity","Pdesign","kW","3.50","5.00"]
["","Energy efficiency class","","","A","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","3.32","4.36"]
["","SCOP/A","","","4.74","4.24"]
["","Energy efficiency class","","","A++","A+"]
["","Annual energy consumption","","kWh/a","981","1,442"]
["Piping connections","Liquid","OD","mm","6.35","6.35"]
["","Gas","OD","mm","9.5","12.7"]
["Nominal efficiency","EER","","","3.58","3.55"]
["","Annual energy consumption","","kWh","475","705"]
["","COP","","","3.41","3.70"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","B","A"]
["Heating capacity","Nom.","","kW","4.20","6.00"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]