{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":118,"n_cols":9,"rows_kept":118,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F"]
[]
[]
[]
[]
["","","","","","FCQHG71FVEB","FCQHG100FVEB","FCQHG125FVEB","FCQHG140FVEB"]
["Sound pressure level","Heating","","High","dBA","","44","45","45"]
["","","","Nom.","dBA","","39","40","41"]
["","","","Low","dBA","","33","35","37"]
["","Cooling","","Low","dBA","","33","35","37"]
["","","","High","dBA","","44","45","45"]
["","","","Nom.","dBA","","39","40","41"]
["Standard Accessories","Operation manual","","","","Operation manual","Operation manual","Operation manual","Operation manual"]
["","Installation manual","","","","Installation manual","Installation manual","Installation manual","Installation manual"]
["","Drain hose","","","","Drain hose","Drain hose","Drain hose","Drain hose"]
["","Clamp for drain hose","","","","Clamp for drain hose","Clamp for drain hose","Clamp for drain hose","Clamp for drain hose"]
["","Washer for hanger bracket","","","","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket"]
["","Screws","","","","Screws","Screws","Screws","Screws"]
["","Installation guide","","","","Installation guide","Installation guide","Installation guide","Installation guide"]
["","Insulation for fitting","","","","2","2","2","2"]
["","Sealing pads","","","","4","4","4","4"]
["","Drain sealing pad","","","","Drain sealing pad","Drain sealing pad","Drain sealing pad","Drain sealing pad"]
["","Clamps","","","","Clamps","Clamps","Clamps","Clamps"]
["Control systems","Wired remote control","","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","","","BRC7FA532F","BRC7FA532F","BRC7FA532F"]
["Piping connections","Liquid","","OD","mm","","9.52","9.52","9.52"]
["","Gas","","OD","mm","","15.9","15.9","15.9"]
["","Drain","","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Decoration panel 4","Dimensions","","Depth","mm","","50","50","50"]
["","","","Width","mm","","950","950","950"]
["","","","Height","mm","","950","950","950"]
["","Model","","","","","BYCQ140D7W1 - white with grey louvers","BYCQ140D7W1 - white with grey louvers","BYCQ140D7W1 - white with grey louvers"]
["","Colour","","","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["","Weight","","","kg","","5.4","5.4","5.4"]
["Sound power level","Cooling","","","dBA","","61","61","61"]
["","Heating","","","dBA","","61","61","61"]
["Dimensions","Unit","","Width","mm","","840","840","840"]
["","","","Depth","mm","","840","840","840"]
["","","","Height","mm","","288","288","288"]
["Casing","Material","","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["Weight","Unit","","","kg","","26","26","26"]
["Decoration panel 2","Weight","","","kg","","10.3","10.3","10.3"]
["","Model","","","","","BYCQ140D7GW1 - auto cleaning panel","BYCQ140D7GW1 - auto cleaning panel","BYCQ140D7GW1 - auto cleaning panel"]
["","Dimensions","","Depth","mm","","950","950","950"]
["","","","Width","mm","","950","950","950"]
["","","","Height","mm","","130","130","130"]
["","Colour","","","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["Decoration panel 3","Dimensions","","Depth","mm","","950","950","950"]
["","","","Height","mm","","50","50","50"]
["","","","Width","mm","","950","950","950"]
["","Colour","","","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["","Model","","","","","BYCQ140D7W1W - full white","BYCQ140D7W1W - full white","BYCQ140D7W1W - full white"]
["","Weight","","","kg","","5.4","5.4","5.4"]
["Decoration panel","Weight","","","kg","","10.3","10.3","10.3"]
["","Model","","","","","BYCQ140D7GFW1 - auto cleaning panel with fine mesh filter","BYCQ140D7GFW1 - auto cleaning panel with fine mesh filter","BYCQ140D7GFW1 - auto cleaning panel with fine mesh filter"]
["","Dimensions","","Height","mm","","130","130","130"]
["","","","Depth","mm","","950","950","950"]
["","","","Width","mm","","950","950","950"]
["","Colour","","","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["Power supply","Phase","","","","","1~","1~","1~"]
["","Name","","","","","VE","VE","VE"]
["","Frequency","","","Hz","","50","50","50"]
["","Voltage","","","V","","220-240","220-240","220-240"]
["Notes","","","","","","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates."]
["","","","","","","(2) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt.","(2) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt.","(2) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt."]
["","","","","","","(3) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel.","(3) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel.","(3) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel."]
["Casing","Material","","","","Galvanised steel plate"]
["Dimensions","Unit","","Height","mm","288"]
["","","","Width","mm","840"]
["","","","Depth","mm","840"]
["Weight","Unit","","","kg","25"]
["Fan","Air flow rate","Cooling","High","m³/min","21.2"]
["","","","Nom.","m³/min","16.7"]
["","","","Low","m³/min","12.2"]
["","","Heating","High","m³/min","21.2"]
["","","","Nom.","m³/min","16.7"]
["","","","Low","m³/min","12.2"]
["Sound power level","Cooling","","","dBA","53"]
["","Heating","","","dBA","53"]
["Sound pressure level","Cooling","","High","dBA","36"]
["","","","Nom.","dBA","33"]
["","","","Low","dBA","29"]
["","Heating","","High","dBA","36"]
["","","","Nom.","dBA","33"]
["","","","Low","dBA","29"]
["Piping connections","Liquid","","OD","mm","9.52"]
["","Gas","","OD","mm","15.9"]
["","Drain","","","","VP25 (I.D. 25/O.D. 32)"]
["Decoration panel","Model","","","","BYCQ140D7GFW1 - auto cleaning panel with fine mesh filter"]
["","Colour","","","","Pure White (RAL 9010)"]
["","Dimensions","","Height","mm","130"]
["","","","Width","mm","950"]
["","","","Depth","mm","950"]
["","Weight","","","kg","10.3"]
["Decoration panel 2","Model","","","","BYCQ140D7GW1 - auto cleaning panel"]
["","Colour","","","","Pure White (RAL 9010)"]
["","Dimensions","","Height","mm","130"]
["","","","Width","mm","950"]
["","","","Depth","mm","950"]
["","Weight","","","kg","10.3"]
["Decoration panel 3","Model","","","","BYCQ140D7W1W - full white"]
["","Colour","","","","Pure White (RAL 9010)"]
["","Dimensions","","Height","mm","50"]
["","","","Width","mm","950"]
["","","","Depth","mm","950"]
["","Weight","","","kg","5.4"]
["Decoration panel 4","Model","","","","BYCQ140D7W1 - white with grey louvers"]
["","Colour","","","","Pure White (RAL 9010)"]
["","Dimensions","","Height","mm","950"]
["","","","Width","mm","950"]
["","","","Depth","mm","50"]
["","Weight","","","kg","5.4"]
["Control systems","Infrared remote control","","","","BRC7FA532F"]
["","Wired remote control","","","","BRC1D52, BRC1E52A/B"]
["Power supply","Name","","","","VE"]
["","Phase","","","","1~"]
["","Power supply-=-Frequency","","Frequency","","50"]
["","Power supply-=-Voltage","","Voltage","","220-240"]