{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":11,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDM-JV1 / RD-JV1/JY1"]
[]
[]
[]
[]
["","","","","FDM20JEV1K / RD20JEV1K","FDM25JEV1K / RD25JEV1K","FDM30JEV1K / RD30JEV1K","FDM40JEV1K / RD40JEV1K","FDM40JEV1K / RD40JEY1K","FDM50JEV1K / RD50JEY1K","FDM60JEV1K / RD60JEY1K"]
["Piping connections","Liquid","OD","mm","6.35","9.52","9.52","9.52","9.52","9.52","12.7"]
["","Gas","OD","mm","15.88","15.88","15.88","19.05","19.05","19.05","19.05"]
["Nominal efficiency","EER","","","3.47 (6)","2.77 (6)","2.74 (6)","2.92 (6)","3.02 (6)","2.83 (6)","2.90 (6)"]
["","Annual energy consumption","","kWh","780","1,295","1,650","1,850","1,790","2,620","2,972"]
["","Energy labeling Directive","Cooling","","A","D","D","C","B","C","C"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB"]
["","","","","(4) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(4) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(4) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(4) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(4) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(4) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(4) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB"]
["","","","","(5) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 35 DEG C OD DB (HIGH FAN)","(5) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 35 DEG C OD DB (HIGH FAN)","(5) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 35 DEG C OD DB (HIGH FAN)","(5) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 35 DEG C OD DB (HIGH FAN)","(5) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 35 DEG C OD DB (HIGH FAN)","(5) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 35 DEG C OD DB (HIGH FAN)","(5) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 35 DEG C OD DB (HIGH FAN)"]
["","","","","(6) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 46 DEG C OD DB (HIGH FAN)","(6) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 46 DEG C OD DB (HIGH FAN)","(6) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 46 DEG C OD DB (HIGH FAN)","(6) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 46 DEG C OD DB (HIGH FAN)","(6) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 46 DEG C OD DB (HIGH FAN)","(6) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 46 DEG C OD DB (HIGH FAN)","(6) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 46 DEG C OD DB (HIGH FAN)"]
["","","","","(7) - EER IS CALCULATED BASED ON GROSS CAPACITY","(7) - EER IS CALCULATED BASED ON GROSS CAPACITY","(7) - EER IS CALCULATED BASED ON GROSS CAPACITY","(7) - EER IS CALCULATED BASED ON GROSS CAPACITY","(7) - EER IS CALCULATED BASED ON GROSS CAPACITY","(7) - EER IS CALCULATED BASED ON GROSS CAPACITY","(7) - EER IS CALCULATED BASED ON GROSS CAPACITY"]
["","","","","(8) - All units are being tested and comply to ISO 5151 (Non-ducted unit)","(8) - All units are being tested and comply to ISO 5151 (Non-ducted unit)","(8) - All units are being tested and comply to ISO 5151 (Non-ducted unit)","(8) - All units are being tested and comply to ISO 5151 (Non-ducted unit)","(8) - All units are being tested and comply to ISO 5151 (Non-ducted unit)","(8) - All units are being tested and comply to ISO 5151 (Non-ducted unit)","(8) - All units are being tested and comply to ISO 5151 (Non-ducted unit)"]
["","","","","(9) - All specifications are subjected to change by the manufacturer without prior notice.","(9) - All specifications are subjected to change by the manufacturer without prior notice.","(9) - All specifications are subjected to change by the manufacturer without prior notice.","(9) - All specifications are subjected to change by the manufacturer without prior notice.","(9) - All specifications are subjected to change by the manufacturer without prior notice.","(9) - All specifications are subjected to change by the manufacturer without prior notice.","(9) - All specifications are subjected to change by the manufacturer without prior notice."]
["","","","","(10) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(10) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(10) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(10) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(10) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(10) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(10) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]