{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":10,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDM-JV1"]
[]
[]
[]
[]
["","","","","FDM20JEV1K","FDM25JEV1K","FDM30JEV1K","FDM40JEV1K","FDM50JEV1K","FDM60JEV1K"]
["Sound pressure level","Cooling","Low","dBA","38","38","39","44","52","54"]
["","","High","dBA","40","41","45","46","55","58"]
["","","Nom.","dBA","39","40","44","45","53","56"]
["Piping connections","Drain","","","19.1","19.1","19.1","19.1","19.1","19.1"]
["Dimensions","Unit","Width","mm","1,065","1,200","1,228","1,228","1,299","1,499"]
["","","Depth","mm","411","411","420","420","541","541"]
["","","Height","mm","261","261","292","292","378","378"]
["Casing","Colour","","","Without powder paint","Without powder paint","Without powder paint","Without powder paint","Without powder paint","Without powder paint"]
["Weight","Unit","","kg","24","26","32","32","54","62"]
["Fan","External static pressure","High","Pa","40","50","50","50","50","50"]
["","","Nom.","Pa","38","46","50","50","50","50"]
["","","Low","Pa","35","36","50","50","50","50"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","Hz","50","50","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - All units are being tested and comply to ISO 5151 (Non-ducted unit)","(1) - All units are being tested and comply to ISO 5151 (Non-ducted unit)","(1) - All units are being tested and comply to ISO 5151 (Non-ducted unit)","(1) - All units are being tested and comply to ISO 5151 (Non-ducted unit)","(1) - All units are being tested and comply to ISO 5151 (Non-ducted unit)","(1) - All units are being tested and comply to ISO 5151 (Non-ducted unit)"]
["","","","","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice."]
["","","","","(3) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 35 DEG C OD DB (HIGH FAN)","(3) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 35 DEG C OD DB (HIGH FAN)","(3) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 35 DEG C OD DB (HIGH FAN)","(3) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 35 DEG C OD DB (HIGH FAN)","(3) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 35 DEG C OD DB (HIGH FAN)","(3) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 35 DEG C OD DB (HIGH FAN)"]
["","","","","(4) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 46 DEG C OD DB (HIGH FAN)","(4) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 46 DEG C OD DB (HIGH FAN)","(4) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 46 DEG C OD DB (HIGH FAN)","(4) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 46 DEG C OD DB (HIGH FAN)","(4) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 46 DEG C OD DB (HIGH FAN)","(4) - GROSS CAPACITY BASED @ 27/19 DEG C ID DB/WB & 46 DEG C OD DB (HIGH FAN)"]
["","","","","(5) - EER IS CALCULATED BASED ON GROSS CAPACITY","(5) - EER IS CALCULATED BASED ON GROSS CAPACITY","(5) - EER IS CALCULATED BASED ON GROSS CAPACITY","(5) - EER IS CALCULATED BASED ON GROSS CAPACITY","(5) - EER IS CALCULATED BASED ON GROSS CAPACITY","(5) - EER IS CALCULATED BASED ON GROSS CAPACITY"]