{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDM-PV1 / R-PV1/P1"]
[]
[]
[]
[]
["","","","","FDM36PEV1K / R36PEY1K","FDM42PEV1K / R42PEY1K","FDM48PEV1K / R48PEY1K","FDM24PEV1K / R24PEV1K","FDM30PEV1K / R30PEV1K"]
["Cooling capacity","Nom.","","kW","9.7","11.3","13.0","6.8","7.7"]
["Piping connections","Liquid","OD","mm","","","","9.52","9.52"]
["","Gas","OD","mm","","","","15.9","15.9"]
["Nominal efficiency","EER","","","2.49 (1), 8.46 (2)","2.46 (1), 8.39 (2)","2.40 (1), 8.22 (2)","2.72 (1), 9.28 (2)","2.64 (1), 9.01 (2)"]
["","Annual energy consumption","","kWh","1,950","2,300","2,700","1,250","1,460"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1"]
["","","","","(2) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1, Btu/h","(2) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1, Btu/h","(2) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1, Btu/h","(2) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1, Btu/h","(2) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1, Btu/h"]
["","","","","(3) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3","(3) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3","(3) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3","(3) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3","(3) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3"]
["","","","","(4) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3, Btu/h","(4) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3, Btu/h","(4) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3, Btu/h","(4) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3, Btu/h","(4) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3, Btu/h"]
["","","","","(5) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(5) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(5) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(5) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(5) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["Piping connections","Liquid","OD","mm","12.7","12.7","12.7"]
["","Gas","OD","mm","19.1","19.1","19.1"]