{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":9,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDM-PV1"]
[]
[]
[]
[]
["","","","","FDM24PEV1K","FDM30PEV1K","FDM36PEV1K","FDM42PEV1K","FDM48PEV1K"]
["Sound pressure level","Cooling","High","dBA","43","43","53","53","54"]
["","","Nom.","dBA","40","40","48","48","48"]
["Dimensions","Unit","Width","mm","1,270","1,270","1,226","1,226","1,226"]
["","","Depth","mm","504","504","744","744","744"]
["","","Height","mm","268","268","290","290","290"]
["Weight","Unit","","kg","36","36","53","53","55"]
["Fan","External static pressure","High","Pa","120","120","150","150","150"]
["","","Low","Pa","40","40","60","50","50"]
["Power supply","Phase","","","1~","1~","1~","1~","1~"]
["","Name","","","V1","V1","V1","V1","V1"]
["","Frequency","","Hz","50","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240","220-240"]