{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-LV1/LY1"]
[]
[]
[]
[]
["","","","","FDQ125C7VEB / RZQSG125L7V1B","FDQ125C7VEB / RZQSG125L7Y1B9","FDQ125C7VEB / RZQSG125L7Y1B"]
["Cooling capacity","Nom.","","kW","12.0","12.0","12.0 (3)"]
["Space cooling","SEER","","","4.35","4.35","4.35 (6)"]
["","Annual energy consumption","","kWh/a","965.517","965.517"]
["","Capacity","Pdesign","kW","12.00","12.00"]
["","Energy efficiency class","","","C","C"]
["Space heating (Average climate)","Capacity","Pdesign","kW","7.60","7.60"]
["","SCOP/A","","","3.81","3.81","3.81 (6)"]
["","Energy efficiency class","","","A","A"]
["","Annual energy consumption","","kWh/a","2,791","2,791"]
["Nominal efficiency","EER","","","3.21","3.21","3.21"]
["","Annual energy consumption","","kWh","1,870","1,600","1,870"]
["","COP","","","3.51","3.51","3.51"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","B","B","B"]
["Heating capacity","Nom.","","kW","13.5","13.5","13.5 (4)"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m"]
["","","","","","","(5) - Annual energy consumption is according to Energy labeling directive 2002/31/EC"]
["","","","","","","(6) - SEER and SCOP are according to EN 14825"]
["","","","","","","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]