{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":8,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDYB-C / RY-CY1"]
[]
[]
[]
[]
["","","","","FDYB90CV1M / RY90CY1M","FDYB125CY1M / RY125CY1M","FDYB140CV1M / RY140CY1M","FDYB160CV1M / RY160CY1M"]
["Cooling capacity","Nom.","","kW","8.792 (1)","11.723 (1)","14.654 (1)","16.410 (1)"]
["Piping connections","Liquid","OD","mm","9.52","9.52","9.52","12.7"]
["","Gas","OD","mm","15.9","19.1","19.1","19.1"]
["Nominal efficiency","EER","","","2.84","3.22","2.89","2.79"]
["","Annual energy consumption","","kWh","1,548","1,822","2,535","2,942"]
["","COP","","","2.87","3.50","3.47","3.38"]
["","Energy labeling Directive","Cooling","","C","A","C","D"]
["","","Heating","","D","B","B","C"]
["Heating capacity","Nom.","","kW","8.792 (1)","11.723 (1)","15.533 (1)","16.410 (1)"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]