{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":12,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDYB-C"]
[]
[]
[]
[]
["","","","","FDYB30CV1M","FDYB40CV1M","FDYB60CV1M","FDYB71CV1M","FDYB90CV1M","FDYB125CV1M","FDYB140CV1M","FDYB160CV1M"]
["Sound pressure level","Cooling","Super high","dBA","","","","","49","51","53","55"]
["","","Low","dBA","26","29","34","36","38","41","47","47"]
["","","High","dBA","33","37","38","40","46","49","52","53"]
["","","Nom.","dBA","30","34","36","39","42","45","50","50"]
["Standard Accessories","SLM wired handset","","","SLM wired handset","SLM wired handset","SLM wired handset","SLM wired handset","SLM wired handset","SLM wired handset","SLM wired handset","SLM wired handset"]
["Sound power level","Cooling","","dBA","57","61","65","66","73","76","76","78"]
["Dimensions","Unit","Width","mm","765","765","1,065","1,200","929","1,045","1,299","1,499"]
["","","Depth","mm","411","411","411","411","541","541","541","541"]
["","","Height","mm","261","261","261","261","378","378","378","378"]
["Casing","Material","","","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel"]
["","Colour","","","Without powder paint","Without powder paint","Without powder paint","Without powder paint","Without powder paint","Without powder paint","Without powder paint","Without powder paint"]
["Weight","Unit","","kg","17","21","22","25","39","42","54","62"]
["Fan","External static pressure","High","Pa","20","20","29","25","39","39","59","49"]
["","","Nom.","Pa","9.8","9.8","20","15","29","29","39","29"]
["","","Low","Pa","4.9","4.9","9.8","5","20","20","20","20"]
["","","Super high","Pa","","","","","49","49","78","69"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Name","","","V1","V1","V1","V1","V1","V1","V1","V1"]
["","Frequency","","Hz","50","50","50","50","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - Sound power: test with 5ft length discharge duct, terminated flush with internal wall of reverberation room.","(1) - Sound power: test with 5ft length discharge duct, terminated flush with internal wall of reverberation room.","(1) - Sound power: test with 5ft length discharge duct, terminated flush with internal wall of reverberation room.","(1) - Sound power: test with 5ft length discharge duct, terminated flush with internal wall of reverberation room.","(1) - Sound power: test with 5ft length discharge duct, terminated flush with internal wall of reverberation room.","(1) - Sound power: test with 5ft length discharge duct, terminated flush with internal wall of reverberation room.","(1) - Sound power: test with 5ft length discharge duct, terminated flush with internal wall of reverberation room.","(1) - Sound power: test with 5ft length discharge duct, terminated flush with internal wall of reverberation room."]
["","","","","(2) - Sound pressure: tested with 2m length duct at the air discharge outlet and air return inlet (1.4m below the centre of the unit).","(2) - Sound pressure: tested with 2m length duct at the air discharge outlet and air return inlet (1.4m below the centre of the unit).","(2) - Sound pressure: tested with 2m length duct at the air discharge outlet and air return inlet (1.4m below the centre of the unit).","(2) - Sound pressure: tested with 2m length duct at the air discharge outlet and air return inlet (1.4m below the centre of the unit).","(2) - Sound pressure: tested with 2m length duct at the air discharge outlet and air return inlet (1.4m below the centre of the unit).","(2) - Sound pressure: tested with 2m length duct at the air discharge outlet and air return inlet (1.4m below the centre of the unit).","(2) - Sound pressure: tested with 2m length duct at the air discharge outlet and air return inlet (1.4m below the centre of the unit).","(2) - Sound pressure: tested with 2m length duct at the air discharge outlet and air return inlet (1.4m below the centre of the unit)."]
["","","","","(3) - All units are being tested and comply to ISO5151:1994(E).","(3) - All units are being tested and comply to ISO5151:1994(E).","(3) - All units are being tested and comply to ISO5151:1994(E).","(3) - All units are being tested and comply to ISO5151:1994(E).","(3) - All units are being tested and comply to ISO5151:1994(E).","(3) - All units are being tested and comply to ISO5151:1994(E).","(3) - All units are being tested and comply to ISO5151:1994(E).","(3) - All units are being tested and comply to ISO5151:1994(E)."]