{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":16,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDYM-C / RY-CV1"]
[]
[]
[]
[]
["","","","","FDYM30CV1M / RY30CV1M","FDYM40CV1M / RY40CV1M","FDYM60CV1M / RY60CV1M","FDYM71CV1M / RY71CV1M","FDYM80CV1M / RY80CV1M","FDYM90CV1M / RY80CV1M","FDYM80CV1M / RY90CV1M","FDYM90CV1M / RY90CV1M","FDYM100CV1M / RY100CV1M","FDYM125CV1M / RY100CV1M","FDYM100CV1M / RY125CV1M","FDYM125CV1M / RY125CV1M"]
["Cooling capacity","Nom.","","kW","2.780 (1)","3.600 (1)","5.570 (1)","6.890 (1)","7.913 (1)","8.602 (1)","8.792 (1)","8.792 (1)","10.257 (1)","9.818 (1)","11.137 (1)","11.723 (1)"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52","9.52","9.52","9.52","9.52","9.52"]
["","Gas","OD","mm","9.52","12.7","15.9","15.9","15.9","15.9","15.9","15.9","19.1","19.1","19.1","19.1"]
["Nominal efficiency","EER","","","3.09","2.84","2.94","2.63","2.56","2.73","2.85","2.80","3.11","3.01","2.96","3.14"]
["","Annual energy consumption","","kWh","450","634","948","1,308","1,546","1,577","1,545","1,573","1,652","1,633","1,883","1,864"]
["","COP","","","3.52","3.39","3.14","2.77","3.11","3.11","2.87","2.82","3.19","3.14","3.25","3.62"]
["","Energy labeling Directive","Cooling","","B","C","C","D","E","D","C","D","B","B","C","B"]
["","","Heating","","B","C","D","E","D","D","D","D","D","D","C","A"]
["Heating capacity","Nom.","","kW","2.780 (1)","3.600 (1)","5.800 (1)","7.030 (1)","8.206 (1)","8.499 (1)","8.792 (1)","8.79 (1)","10.550 (1)","10.257 (1)","11.280 (1)","11.723 (1)"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]