{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":10,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-N9"]
[]
[]
[]
[]
["","","","","FFA25A2VEB9 / RXM25N2V1B9","FFA25A2VEB9 / RXM25N5V1B9","FFA35A2VEB9 / RXM35N2V1B9","FFA35A2VEB9 / RXM35N5V1B9","FFA50A2VEB9 / RXM50N2V1B9","FFA60A2VEB9 / RXM60N2V1B9"]
["Cooling capacity","Nom.","","kW","2.50","2.50"]
["Space cooling","SEER","","","6.17","6.17"]
["","Annual energy consumption","","kWh/a","142","142"]
["","Capacity","Pdesign","kW","2.50","2.50"]
["","Energy efficiency class","","","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.31","2.31"]
["","SCOP/A","","","4.24","4.24"]
["","Energy efficiency class","","","A+","A+"]
["","Annual energy consumption","","kWh/a","762","762"]
["Nominal efficiency","EER","","","4.57","4.57"]
["","Annual energy consumption","","kWh","273","273"]
["","COP","","","3.90","3.90"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Heating capacity","Nom.","","kW","3.20","3.20"]
["Notes","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - See separate drawing for operation range","(2) - See separate drawing for operation range","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Outdoor unit","","","","","","RXM35N2V1B9","RXM35N5V1B9","","RXM60N2V1B9"]
["Cooling capacity","Nom.","","kW","","","3.40","3.40","5.00","5.70"]
["Heating capacity","Nom.","","kW","","","4.20","4.20","5.80","7.00"]
["Nominal efficiency","EER","","","","","3.81","3.81","3.24","3.05"]
["","COP","","","","","3.50","3.50","3.49","3.41"]
["","Annual energy consumption","","kWh","","","446","446","772","934"]
["","Energy labeling Directive","Cooling","","","","A","A","A","B"]
["","","Heating","","","","B","B","B","B"]
["Space cooling","Energy efficiency class","","","","","A++","A++","A+","A+"]
["","Capacity","Pdesign","kW","","","3.40","3.40","5.00","5.70"]
["","SEER","","","","","6.38","6.38","5.98","5.76"]
["","Annual energy consumption","","kWh/a","","","186","186","293","347"]
["Space heating (Average climate)","Energy efficiency class","","","","","A+","A+","A","A+"]
["","Capacity","Pdesign","kW","","","3.10","3.10","3.84","3.96"]
["","SCOP/A","","","","","4.10","4.10","3.90","4.04"]
["","Pdh Heating capacity at -10°","","kW","","","2.04","2.04","3.40","3.66"]
["","Annual energy consumption","","kWh/a","","","1058","1058","1378","1372"]
["Energy Efficiency Range","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]