{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":13,"n_cols":10,"rows_kept":13,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHC-JV1 / RD-JV1/JY1"]
[]
[]
[]
[]
["","","","","FHC20JEV1K / RD20JEV1K","FHC25JEV1K / RD25JEV1K","FHC30JEV1K / RD30JEV1K","FHC40JEV1K / RD40JEV1K","FHC40JEV1K / RD40JEY1K","FHC50JEV1K / RD50JEY1K"]
["Cooling capacity","Nom.","","kW","5.280 (3)","7.030 (3)","8.790 (3)","10.550 (3)","10.550 (3)","14.070 (3)"]
["Piping connections","Liquid","OD","mm","6.35","9.52","9.52","9.52","9.52","9.52"]
["","Gas","OD","mm","15.88","15.88","15.88","19.05","19.05","19.05"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB"]
["","","","","(4) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit).","(4) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit).","(4) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit).","(4) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit).","(4) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit).","(4) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit)."]