{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHYC-JVL / RYD-JVL/JTL/JYL"]
[]
[]
[]
[]
["","","","","FHYC20JEVLK / RYD20JEVLK","FHYC25JEVLK / RYD25JEVLK","FHYC30JEVLK / RYD30JEVLK","FHYC40JEVLK / RYD40JEVLK","FHYC50JEVLK / RYD50JETLK"]
["Cooling capacity","Nom.","","kW","5.720","6.830","8.210","10.550","13.920"]
["Nominal efficiency","EER","","","2.77","2.64","2.64","2.63","2.58"]
["","Annual energy consumption","","kWh","1,030","1,295","1,555","2,005","2,690"]
["","COP","","","3.26","3.12","3.40","3.08","2.92"]
["","Energy labeling Directive","Cooling","","D","D","D","D","E"]
["","","Heating","","C","D","C","D","D"]
["Heating capacity","Nom.","","kW","5.860 (4)","7.180 (4)","8.790 (4)","11.250 (4)","14.650 (4)"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 8°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 8°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 8°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 8°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 8°CDB, 6°CWB"]
["","","","","(5) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit).","(5) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit).","(5) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit).","(5) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit).","(5) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit)."]
["","","","","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]