{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHYC-JVL"]
[]
[]
[]
[]
["","","","","FHYC20JEVLK","FHYC25JEVLK","FHYC30JEVLK","FHYC40JEVLK","FHYC50JEVLK"]
["Sound pressure level","Heating","High","dBA","34","37","43","46","49"]
["","","Nom.","dBA","32","34","41","43","46"]
["","","Silent operation","dBA","28","32","35","36","41"]
["","","Low","dBA","30","33","38","40","45"]
["","Cooling","Silent operation","dBA","28","32","35","36","41"]
["","","Low","dBA","30","33","38","40","45"]
["","","High","dBA","34","37","43","46","49"]
["","","Nom.","dBA","32","34","41","43","46"]
["Piping connections","Drain","","","19.05","19.05","19.05","19.05","19.05"]
["Dimensions","Unit","Width","mm","820","820","820","820","820"]
["","","Depth","mm","820","820","820","820","820"]
["","","Height","mm","265","265","265","300","300"]
["Casing","Colour","","","Unpainted","Unpainted","Unpainted","Unpainted","Unpainted"]
["Weight","Unit","","kg","29","29","29","42","42"]
["Decoration panel","Weight","","kg","6","6","6","6","6"]
["Power supply","Phase","","","1~","1~","1~","1~","1~"]
["","Frequency","","Hz","60","60","60","60","60"]
["","Voltage","","V","220","220","220","220","220"]