{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9 / RXM-N9"]
[]
[]
[]
[]
["","","","","FNA25A2VEB9 / RXM25N5V1B9","FNA25A2VEB9 / RXM25N2V1B9","FNA35A2VEB9 / RXM35N2V1B9","FNA35A2VEB9 / RXM35N5V1B9","FNA50A2VEB9 / RXM50N2V1B9","FNA60A2VEB9 / RXM60N2V1B9"]
["Cooling capacity","Nom.","","kW","2.60","2.60","3.40","3.40","5.00","6.00"]
["Space cooling","SEER","","","5.68","5.68","5.70","5.70","5.77","5.56"]
["","Annual energy consumption","","kWh/a","160","160","209","209","303","378"]
["","Capacity","Pdesign","kW","2.60","2.60","3.40","3.40","5.00","6.00"]
["","Energy efficiency class","","","A+","A+","A+","A+","A+","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.80","2.80","2.90","2.90","4.00","4.60"]
["","SCOP/A","","","4.24","4.24","4.05","4.05","4.09","4.16"]
["","Energy efficiency class","","","A+","A+","A+","A+","A+","A+"]
["","Annual energy consumption","","kWh/a","924","924","1,002","1,002","1,368","1,547"]
["Nominal efficiency","EER","","","3.80","3.80","3.09","3.09","3.38","2.70"]
["","Annual energy consumption","","kWh","342","342","550","550","740","1,111"]
["","COP","","","4.00","4.00","3.48","3.48","3.34","3.11"]
["","Energy labeling Directive","Cooling","","A","A","B","B","A","D"]
["","","Heating","","A","A","B","B","C","D"]
["Heating capacity","Nom.","","kW","3.20","3.20","4.00","4.00","5.80","7.00"]
["Notes","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - See separate drawing for operation range","(2) - See separate drawing for operation range","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]