{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":10,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9 / RXM-R"]
[]
[]
[]
[]
["","","","","FNA25A2VEB9 / RXM25R5V1B","FNA35A2VEB9 / RXM35R5V1B","FNA50A2VEB9 / RXM50R2V1B","FNA50A2VEB9 / RXM50R5V1B","FNA60A2VEB9 / RXM60R5V1B","FNA60A2VEB9 / RXM60R2V1B"]
["Cooling capacity","Nom.","","kW","2.60","3.40","5.00","5.00","6.00","6.00"]
["Heating capacity","Nom.","","kW","3.20","4.00","5.80","5.80","7.00","7.00"]
["Nominal efficiency","Annual energy consumption","","kWh","342","550","740","740","1,111","1,111"]
["","COP","","","4.00","3.48","3.34","3.34","3.11","3.11"]
["","EER","","","3.80","3.09","3.38","3.38","2.70","2.70"]
["","Energy labeling Directive","Cooling","","A","B","A","A","D","D"]
["","","Heating","","A","B","C","C","D","D"]
["Space cooling","Annual energy consumption","","kWh/a","160","209","303","303","378","378"]
["","Energy efficiency class","","","A+","A+","A+","A+","A","A"]
["","Capacity","Pdesign","kW","2.60","3.40","5.00","5.00","6.00","6.00"]
["","SEER","","","5.68","5.70","5.77","5.77","5.56","5.56"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","924","1,002","1,368","1,368","1,547","1,547"]
["","Capacity","Pdesign","kW","2.80","2.90","4.00","4.00","4.60","4.60"]
["","Energy efficiency class","","","A+","A+","A+","A+","A+","A+"]
["","Pdh Heating capacity at -10°","","kW","2.16","","3.54","3.54","3.94","3.94"]
["","SCOP/A","","","4.24","4.05","4.09","4.09","4.16","4.16"]
["Notes","","","","(1) - See separate drawing for electrical data","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - See separate drawing for operation range","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]