{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9 / RXM-R9"]
[]
[]
[]
[]
["","","","","FNA25A2VEB9 / RXM25R5V1B9","FNA35A2VEB9 / RXM35R5V1B9"]
["Cooling capacity","Nom.","","kW","2.60","3.40"]
["Heating capacity","Nom.","","kW","3.20","4.00"]
["Nominal efficiency","Annual energy consumption","","kWh","342","550"]
["","COP","","","4.00","3.48"]
["","EER","","","3.80","3.09"]
["","Energy labeling Directive","Cooling","","A","B"]
["","","Heating","","A","B"]
["Space cooling","Annual energy consumption","","kWh/a","160","209"]
["","Energy efficiency class","","","A+","A+"]
["","Capacity","Pdesign","kW","2.60","3.40"]
["","SEER","","","5.68","5.70"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","924","1,002"]
["","Capacity","Pdesign","kW","2.80","2.90"]
["","Energy efficiency class","","","A+","A+"]
["","Pdh Heating capacity at -10°","","kW","2.16"]
["","SCOP/A","","","4.24","4.05"]
["Notes","","","","(1) - See separate drawing for electrical data","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - See separate drawing for operation range","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - See separate drawing for operation range"]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - See separate drawing for electrical data"]