{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":7,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FT-H / R-H"]
[]
[]
[]
[]
["","","","","FT18HEV1K / R18HEV1K","FT24HEV1K / R24HEV1K","FT28HEV1K / R28HEV1K"]
["Cooling capacity","Nom.","","kW","5.7","6.45","8.82"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gas","OD","mm","12.7","15.9","15.9"]
["Nominal efficiency","EER","","","2.71, 9.25 (3)","2.69, 9.18 (3)","2.90, 9.89 (3)"]
["","Annual energy consumption","","kWh","2,850","3,225","4,410"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]