{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":7,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FT-HL / R-HL"]
[]
[]
[]
[]
["","","","","FT18HEVLK / R18HEVLK","FT24HEVLK / R24HEVLK","FT30HEVLK / R30HEVLK"]
["Cooling capacity","Nom.","","kW","5.45 (1), 4.80 (3)","6.15 (1), 5.30 (3)","8.25 (1), 7.37 (3)"]
["Piping connections","Liquid","OD","mm","6.35","6.35","9.52"]
["","Gas","OD","mm","12.7","15.9","15.9"]
["Nominal efficiency","EER","","","2.49 (1), 8.48 (2), 1.91 (3), 6.50 (4)","2.42 (1), 8.27 (2), 1.79 (3), 6.12 (4)","2.47 (1), 8.43 (2), 1.84 (3), 6.29 (4)"]
["","Annual energy consumption","","kWh","2,725","3,075","4,125"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1"]
["","","","","(2) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1, Btu/h","(2) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1, Btu/h","(2) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1, Btu/h"]
["","","","","(3) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3","(3) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3","(3) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3"]
["","","","","(4) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3, Btu/h","(4) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3, Btu/h","(4) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3, Btu/h"]
["","","","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]