{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":7,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FT-HL"]
[]
[]
[]
[]
["","","","","FT18HEVLK","FT24HEVLK","FT30HEVLK"]
["Sound pressure level","Cooling","Silent operation","dBA","34","34"]
["","","Low","dBA","37","37"]
["","","High","dBA","45","45"]
["","","Nom.","dBA","41","42","44"]
["Dimensions","Unit","Width","mm","940","1,007","1,178"]
["","","Depth","mm","298","219","227"]
["","","Height","mm","200","315","326"]
["Weight","Unit","","kg","13","15.5","17.5"]
["Power supply","Phase","","","1~","1~","1~"]
["","Name","","","VL","VL","VL"]
["","Frequency","","Hz","60","60","60"]
["","Voltage","","V","220","220","220"]