{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTKM-PVM / RKM-PVM"]
[]
[]
[]
[]
["","","","","FTKM18PVMK / RKM18PVMK","FTKM24PVMK / RKM24PVMK","FTKM28PVMK / RKM28PVMK"]
["Cooling capacity","Min.","","kW","1.7","1.9","1.9"]
["","Max.","","kW","6.0","8.6","9.4"]
["","Nom.","","kW","5.28 (1), 5.3 (2)","7.03 (1), 7.0 (2)","8.21 (1), 8.0 (2)"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gas","OD","mm","12.7","12.7","15.9"]
["Nominal efficiency","EER","","","13.33 (3), 8.49 (4)","12.70 (3), 8.51 (4)","12.12 (3), 8.56 (4)"]
["","Annual energy consumption","","kWh","675","945","1,155"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); Standard:T1, Kw","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); Standard:T1, Kw","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); Standard:T1, Kw"]
["","","","","(2) - Cooling: indoor temp. 29°CDB, 19.0°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); Standard:T3, Kw","(2) - Cooling: indoor temp. 29°CDB, 19.0°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); Standard:T3, Kw","(2) - Cooling: indoor temp. 29°CDB, 19.0°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); Standard:T3, Kw"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); Standard:T1, Btu/h","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); Standard:T1, Btu/h","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); Standard:T1, Btu/h"]
["","","","","(4) - Cooling: indoor temp. 29°CDB, 19.0°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); Standard:T3, Btu/h","(4) - Cooling: indoor temp. 29°CDB, 19.0°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); Standard:T3, Btu/h","(4) - Cooling: indoor temp. 29°CDB, 19.0°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); Standard:T3, Btu/h"]
["","","","","(5) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); Standard:T1, kcal/h","(5) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); Standard:T1, kcal/h","(5) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); Standard:T1, kcal/h"]
["","","","","(6) - 220V","(6) - 220V","(6) - 220V"]
["","","","","(7) - 230V","(7) - 230V","(7) - 230V"]
["","","","","(8) - 240V","(8) - 240V","(8) - 240V"]