{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTKM-PVM"]
[]
[]
[]
[]
["","","","","FTKM18PVMK","FTKM24PVMK","FTKM28PVMK"]
["Sound pressure level","Cooling","Silent operation","dBA","32","34","39"]
["","","Low","dBA","35","37","42"]
["","","High","dBA","48","51","54"]
["","","Nom.","dBA","42","45","49"]
["Standard Accessories","Installation manual","","","1","1","1"]
["","Operation manual","","","1","1","1"]
["","Infrared remote control","","","1","1","1"]
["","Batteries","","","2","2","2"]
["","Remote control holder","","","1","1","1"]
["","Mounting plate","","","1","1","1"]
["","Indoor unit fixing screws","","","2","2","3"]
["","Titanium apatite photocatalytic air purification filter","","","2","2","3"]
["","Fixing screws for mounting plate","","","9","9","9"]
["","Fixing screw for remote controller holder","","","2","2","2"]
["","Insulation tape","","","1","1","1"]
["","Screw cover","","","3","3","3"]
["Control systems","Infrared remote control","","","ARC466A25","ARC466A25","ARC466A25"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gas","OD","mm","12.7","12.7","15.9"]
["Dimensions","Unit","Width","mm","1,050","1,050","1,200"]
["","","Depth","mm","259","259","259"]
["","","Height","mm","340","340","340"]
["Casing","Colour","","","White (N-95)","White (N-95)","White (N-95)"]
["Weight","Unit","","kg","15","15","18"]
["Power supply","Phase","","","1~","1~","1~"]
["","Frequency","","Hz","50/60","50/60","50/60"]
["","Voltage","","V","220-240/220-230","220-240/220-230","220-240/220-230"]
["Notes","","","","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V"]