{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":8,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTV-A"]
[]
[]
[]
[]
["","","","","FTV25AV1","FTV35AV1","FTV50AV1","FTV60AV1"]
["Sound pressure level","Cooling","Silent operation","dBA","32","32","37","37"]
["","","Low","dBA","35","35","41","41"]
["","","High","dBA","40","41","47","49"]
["","","Nom.","dBA","37","38","44","45"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.52","12.7","12.7","15.9"]
["Sound power level","Cooling","","dBA","47","48","54","55"]
["Dimensions","Unit","Width","mm","790","845","940","1,007"]
["","","Depth","mm","174","180","200","219"]
["","","Height","mm","265","275","298","315"]
["Weight","Unit","","kg","9","10","13","15.5"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Frequency","","Hz","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240"]