{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":10,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Sound pressure level","Heating","","High","dBA","39","40","41","","46"]
["","","","Medium","dBA","32","33","33","","42"]
["","","","Silent operation","dBA","19","19","19","","24"]
["","","","Low","dBA","25","25","25","","33"]
["","Cooling","","Medium","dBA","32","33","33","","39"]
["","","","Silent operation","dBA","19","19","19","","24"]
["","","","Low","dBA","25","25","25","","31"]
["","","","High","dBA","39","40","41","","46"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","Air filter","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Remote controller mounting plate","","","","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1"]
["","Screw cover","","","","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["Refrigerant","GWP","","","","675.0","675.0","675.0","","675.0"]
["Control systems","Wired remote control","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","","6.35"]
["","Gas","","OD","mm","9.50","9.50","9.50","","12.70"]
["","Drain","","","","18","18","18","","18"]
["Power input","Cooling","","Nom.","kW","0.020","0.022","0.023","","0.030"]
["","Heating","","Nom.","kW","0.020","0.020","0.022","","0.039"]
["Sound power level","Cooling","","","dBA","57","57","60","","60"]
["Dimensions","Unit","","Width","mm","798","798","798","","798"]
["","","","Depth","mm","189","189","189","","189"]
["","","","Height","mm","295","295","295","","295"]
["Casing","Colour","","","","White","White","White","","White"]
["Weight","Unit","","","kg","11.50","11.50","11.50","","11.50"]
["Fan","Air flow rate","Heating","High","m³/min","10.9","11.1","11.5","","15.1"]
["","","","Medium","m³/min","8.7","9.0","9.0","","11.1"]
["","","","Low","m³/min","6.4","6.4","6.4","","8.2"]
["","","","Silent operation","m³/min","4.5","4.5","4.5","","5.7"]
["","","Cooling","Low","m³/min","6.1","6.1","6.1","","7.6"]
["","","","Medium","m³/min","8.2","8.6","8.6","","10.4"]
["","","","High","m³/min","11.0","11.5","11.9","","13.5"]
["","","","Silent operation","m³/min","4.6","4.6","4.6","","5.2"]
["Power supply","Phase","","","","1~","1~","1~","","1~"]
["","Name","","","","V1","V1","V1","","V1"]
["","Frequency","","","Hz","50","50","50","","50"]
["","Voltage","","","V","220-240","220-240","220-240","","220-240"]
["Power input","Cooling","","Nom.","kW","","","","0.028"]
["","Heating","","Nom.","kW","","","","0.036"]
["Casing","Colour","","","","","","","White"]
["Dimensions","Unit","","Height","mm","","","","295"]
["","","","Width","mm","","","","798"]
["","","","Depth","mm","","","","189"]
["Weight","Unit","","","kg","","","","11.50"]
["Fan","Air flow rate","Cooling","High","m³/min","","","","13.1"]
["","","","Medium","m³/min","","","","9.8"]
["","","","Low","m³/min","","","","7.2"]
["","","","Silent operation","m³/min","","","","4.6"]
["","","Heating","High","m³/min","","","","14.6"]
["","","","Medium","m³/min","","","","10.5"]
["","","","Low","m³/min","","","","7.7"]
["","","","Silent operation","m³/min","","","","5.2"]
["Sound power level","Cooling","","","dBA","","","","60"]
["Sound pressure level","Cooling","","High","dBA","","","","45"]
["","","","Medium","dBA","","","","37"]
["","","","Low","dBA","","","","29"]
["","","","Silent operation","dBA","","","","21"]
["","Heating","","High","dBA","","","","45"]
["","","","Medium","dBA","","","","37"]
["","","","Low","dBA","","","","29"]
["","","","Silent operation","dBA","","","","21"]
["Refrigerant","GWP","","","","","","","675.0"]
["Piping connections","Liquid","","OD","mm","","","","6.35"]
["","Gas","","OD","mm","","","","12.70"]
["","Drain","","","","","","","18"]
["Control systems","Infrared remote control","","","","","","","ARC466A58"]
["","Wired remote control","","","","","","","BRC073"]
["Power supply","Name","","","","","","","V1"]
["","Phase","","","","","","","1~"]
["","Frequency","","","Hz","","","","50"]
["","Voltage","","","V","","","","220-240"]