{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":25,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / 2MXM-A"]
[]
[]
[]
[]
["","","","","FTXM20N2V1B / FTXM25N2V1B / 2MXM40A2V1B","FTXM20N2V1B / FTXM35N2V1B / 2MXM40A2V1B","FTXM25N2V1B / FTXM25N2V1B / 2MXM40A2V1B","FTXM25N2V1B / FTXM35N2V1B / 2MXM40A2V1B","FTXM20N2V1B / FTXM20N2V1B / 2MXM40A2V1B","FTXM20N2V1B / FTXM20N2V1B / 2MXM50A2V1B","FTXM20N2V1B / FTXM25N2V1B / 2MXM50A2V1B","FTXM20N2V1B / FTXM35N2V1B / 2MXM50A2V1B","FTXM20N2V1B / FTXM42N2V1B / 2MXM50A2V1B","FTXM20N2V1B / FTXM50N2V1B / 2MXM50A2V1B","FTXM25N2V1B / FTXM35N2V1B / 2MXM50A2V1B","FTXM25N2V1B / FTXM42N2V1B / 2MXM50A2V1B","FTXM25N2V1B / FTXM50N2V1B / 2MXM50A2V1B","FTXM35N2V1B / FTXM35N2V1B / 2MXM50A2V1B","FTXM35N2V1B / FTXM42N2V1B / 2MXM50A2V1B","FTXM35N2V1B / FTXM50N2V1B / 2MXM50A2V1B","FTXM42N2V1B / FTXM42N2V1B / 2MXM50A2V1B","FTXM25N2V1B / FTXM25N2V1B / 2MXM50A2V1B","FTXM20N2V1B / FTXM50N2V1B / 2MXM68A2V1B","FTXM25N2V1B / FTXM42N2V1B / 2MXM68A2V1B","FTXM35N2V1B / FTXM35N2V1B / 2MXM68A2V1B"]
["Cooling capacity","Nom.","","kW","4.00","4.00","4.00","4.00","","4.00","4.50","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00"]
["Space cooling","SEER","","","8.50","8.19","8.36","8.11","","8.71","8.67","8.54","8.54","8.51","8.56","8.58","8.52","8.57","8.60","8.52","8.56"]
["","Annual energy consumption","","kWh/a","165","171","168","173","","161","182","205","205","206","205","204","206","205","204","206","205"]
["","Capacity","Pdesign","kW","4.00","4.00","4.00","4.00","","4.00","4.50","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00"]
["","Energy efficiency class","","","A+++","A++","A++","A++","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","3.20","3.20","3.20","3.20","","4.00","4.10","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20"]
["","SCOP/A","","","4.60","4.60","4.60","4.61","","4.61","4.61","4.61","4.63","4.68","4.62","4.65","4.71","4.66","4.67","4.75","4.70"]
["","Energy efficiency class","","","A++","A++","A++","A++","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Pdh Heating capacity at -10°","","kW","2.56","2.58","2.57","2.59","","3.27","3.33","3.40","3.41","3.51","3.41","3.42","3.53","3.42","3.43","3.54","3.44"]
["","Annual energy consumption","","kWh/a","973","974","974","971","","1,214","1,244","1,275","1,268","1,255","1,272","1,265","1,249","1,262","1,258","1,238","1,251"]
["Nominal efficiency","Annual energy consumption","","kWh","481","476","478","472","","471","534","619","614","608","616","611","605","608","604","598","601"]
["","EER","","","4.16","4.20","4.18","4.24","","4.25","4.21","4.04","4.07","4.11","4.06","4.09","4.13","4.11","4.14","4.18","4.16"]
["","COP","","","4.32","4.41","4.37","4.46","","4.09","4.10","4.12","4.13","4.15","4.05","4.03","3.98","4.01","4.00","3.94","3.98"]
["","Energy labeling Directive","Cooling","","A","A","A","A","","A","A","A","A","A","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","","A","A","A","A","A","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","4.20","4.20","4.20","4.20","","5.20","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Cooling capacity","Nom.","","kW","","","","","4.00","","","","","","","","","","","","","5.00","6.8","6.7","6.8"]
["Heating capacity","Nom.","","kW","","","","","4.20","","","","","","","","","","","","","5.60","8.60","8.30","8.60"]
["Nominal efficiency","EER","","","","","","","4.30","","","","","","","","","","","","","4.01","3.59","3.74","3.94"]
["","COP","","","","","","","4.28","","","","","","","","","","","","","4.08","3.82","3.95","3.81"]
["","Annual energy consumption","","kWh","","","","","465","","","","","","","","","","","","","623","947","896","863"]
["","Energy labeling Directive","Cooling","","","","","","A","","","","","","","","","","","","","A"]
["","","Heating","","","","","","A","","","","","","","","","","","","","A"]
["Space cooling","Energy efficiency class","","","","","","","A+++","","","","","","","","","","","","","A+++","A++","A++","A++"]
["","Capacity","Pdesign","kW","","","","","4.00","","","","","","","","","","","","","5.00","6.80","6.70","6.80"]
["","SEER","","","","","","","8.53","","","","","","","","","","","","","8.53","6.75","6.94","6.97"]
["","Annual energy consumption","","kWh/a","","","","","164","","","","","","","","","","","","","205","353","338","342"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","A++","","","","","","","","","","","","","A++","A","A","A+"]
["","Capacity","Pdesign","kW","","","","","3.20","","","","","","","","","","","","","4.20","4.50","4.30","4.80"]
["","SCOP/A","","","","","","","4.64","","","","","","","","","","","","","4.61","3.90","3.86","4.00"]
["","Pdh Heating capacity at -10°","","kW","","","","","2.55","","","","","","","","","","","","","3.20","3.55","3.41","3.73"]
["","Annual energy consumption","","kWh/a","","","","","966","","","","","","","","","","","","","1275","1614","1560","1680"]
["Energy Efficiency Range","","","","","","","","A+++ ~ D","","","","","","","","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]