{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":7,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTY-H / RY-H"]
[]
[]
[]
[]
["","","","","FTY18HEV1K / RY18HEV1K","FTY24HEV1K / RY24HEV1K","FTY28HEV1K / RY28HEV1K"]
["Cooling capacity","Nom.","","kW","5.4","6.45","8.6"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gas","OD","mm","12.7","15.9","15.9"]
["Nominal efficiency","EER","","","2.70, 9.20 (3)","2.80, 9.57 (3)","2.69, 9.16 (3)"]
["","Annual energy consumption","","kWh","2,700","3,225","4,300"]
["","COP","","","3.08, 10.51 (3)","3.06, 10.47 (3)","2.97, 10.13 (3)"]
["Heating capacity","Nom.","","kW","6.0","7.2","9.2"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(3) - Btu/W","(3) - Btu/W","(3) - Btu/W"]
["","","","","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]