{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":7,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTY-H"]
[]
[]
[]
[]
["","","","","FTY18HEV1K","FTY24HEV1K","FTY28HEV1K"]
["Sound pressure level","Heating","Silent operation","dBA","32","34","44"]
["","","Low","dBA","37","38","46"]
["","Cooling","Silent operation","dBA","32","34","44"]
["","","Low","dBA","37","38","46"]
["","","Nom.","dBA","41","42","49"]
["","Cooling","Nom.","dBA","41","42","49"]
["Dimensions","Unit","Width","mm","940","1,007","1,178"]
["","","Depth","mm","200","219","253"]
["","","Height","mm","298","315","326"]
["Weight","Unit","","kg","13","15.5","17.5"]
["Power supply","Phase","","","1~","1~","1~"]
["","Name","","","V1","V1","V1"]
["","Frequency","","Hz","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240"]