{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTY-HL / RY-HL"]
[]
[]
[]
[]
["","","","","FTY18HEVLK / RY18HEVLK","FTY24HEVLK / RY24HEVLK","FTY30HEVLK / RY30HEVLK"]
["Cooling capacity","Nom.","","kW","5.45 (3), 4.70 (5)","6.25 (3), 5.37 (5)","8.01 (3), 7.10 (5)"]
["Piping connections","Liquid","OD","mm","6.35","6.35","9.52"]
["","Gas","OD","mm","12.7","15.9","15.9"]
["Nominal efficiency","EER","","","2.42, 8.25 (8), 1.79, 6.12 (8)","2.53 (1), 8.64 (8), 1.94, 6.62 (8)","2.43, 8.29 (8), 1.86, 6.35 (8)"]
["","Annual energy consumption","","kWh","2,725","3,125","4,005"]
["","COP","","","3.03, 10.34 (8)","2.82, 9.62 (8)","2.78, 9.49 (8)"]
["Heating capacity","Nom.","","kW","6.45","6.83","8.96"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1","(3) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1","(3) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1"]
["","","","","(4) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1, Btu/h","(4) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1, Btu/h","(4) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal); Standard: T1, Btu/h"]
["","","","","(5) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3","(5) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3","(5) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3"]
["","","","","(6) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3, Btu/h","(6) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3, Btu/h","(6) - Cooling: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°CDB, 24°CWB; equivalent piping length: 7.5m (horizontal); SASO Standard - T3, Btu/h"]
["","","","","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)"]
["","","","","(8) - Btu/W","(8) - Btu/W","(8) - Btu/W"]
["","","","","(9) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(9) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(9) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]